(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(color "Black")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(color "Black")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(aux_axis_origin 138.1125 71.4375)
		(grid_origin 138.1125 71.4375)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk yes)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "gerber/")
		)
	)
	(net 0 "")
	(net 1 "Net-(J1-Pin_4)")
	(net 2 "Net-(J1-Pin_1)")
	(net 3 "Net-(J1-Pin_2)")
	(net 4 "Net-(J1-Pin_3)")
	(footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad"
		(layer "F.Cu")
		(uuid "0252980b-3911-4efa-83ff-4ee7d78cf941")
		(at 256.1125 29.4375)
		(descr "Mounting Hole 3.2mm, M3, DIN965")
		(tags "mounting hole 3.2mm m3 din965")
		(property "Reference" "REF**"
			(at -4.97 -0.037 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "854b86ef-a931-4af4-97b9-e201aa270040")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "MountingHole_3.2mm_M3_DIN965_Pad"
			(at 0 3.8 0)
			(layer "F.Fab")
			(uuid "6e387279-5706-4d85-96f9-ae2ea7268fdc")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "5f3cfa97-7b47-4452-b7e6-86292372bd34")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3f9e91f1-36fc-419a-ade2-061471064d32")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "61d270ac-98ba-4821-b5cf-f0a03e7967c8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_circle
			(center 0 0)
			(end 2.8 0)
			(stroke
				(width 0.15)
				(type solid)
			)
			(fill none)
			(layer "Cmts.User")
			(uuid "aab1a28f-2b28-49b0-bba8-f29766f7a71d")
		)
		(fp_circle
			(center 0 0)
			(end 3.05 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill none)
			(layer "F.CrtYd")
			(uuid "81325b01-1eb2-4644-a0ee-aa7732222cb1")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "bede16c5-de63-4be0-8ffe-f1b3e05bba9f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 5.6 5.6)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(uuid "cd11a670-7417-4e8b-8fb4-73ff8637a7ed")
		)
	)
	(footprint "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
		(layer "F.Cu")
		(uuid "06dbdf9e-7d71-45d1-9669-a674b5ffd2d3")
		(at 185.7375 42.8625)
		(property "Reference" "MX9"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
			(uuid "ce3d4145-85da-424d-b95f-401f63c0d87e")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "MX_SW_HS"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "d69bc69f-2bd5-42d1-9b88-ee8df74e2cbd")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "d3ffb1b2-b9e1-498e-aa31-5c93ec6cacb1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "742e4501-41f7-4164-831b-eedd3235697c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted, Kailh CPG151101S11 for Cherry MX style switches"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "7229f4c2-e3e6-4154-a8c4-ad4459879301")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/04b4c660-9ebf-439b-a319-bb41158f2727")
		(sheetname "Stammblatt")
		(sheetfile "geebord-plate.kicad_sch")
		(attr exclude_from_pos_files allow_missing_courtyard)
		(fp_rect
			(start -9.525 -9.525)
			(end 9.525 9.525)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "Dwgs.User")
			(uuid "2026fc80-6bb2-49b1-a3fe-a92451dbafbc")
		)
		(fp_line
			(start -7 -6.5)
			(end -7 6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "0b818784-0f90-44f4-8c98-bb3a916303ee")
		)
		(fp_line
			(start -6.5 7)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "6eaac8e7-3bba-4ac8-b80e-8595057d8a65")
		)
		(fp_line
			(start 6.5 -7)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "99452a11-a50b-4a23-bf58-80b0e5d01809")
		)
		(fp_line
			(start 7 6.5)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "4cd05534-5412-47dd-a04a-7ce967c09d23")
		)
		(fp_arc
			(start -7 -6.5)
			(mid -6.853553 -6.853553)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "46cb516b-acd2-40d6-ae5d-b9c3083d34b9")
		)
		(fp_arc
			(start -6.497236 6.998884)
			(mid -6.850789 6.852437)
			(end -6.997236 6.498884)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "20d0a2f6-2e5e-4835-8efe-77271a03cb56")
		)
		(fp_arc
			(start 6.5 -7)
			(mid 6.853553 -6.853553)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "1745ec42-a1dd-485d-bf6e-34c0fe6ff405")
		)
		(fp_arc
			(start 7 6.5)
			(mid 6.853553 6.853553)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "d8689e76-8077-44c6-8ad1-3f72a0e24c85")
		)
	)
	(footprint "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
		(layer "F.Cu")
		(uuid "0ee1be56-f27f-4b10-a0de-ebd5935fc2b9")
		(at 242.8875 100.0125)
		(property "Reference" "MX46"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
			(uuid "2c4b08f0-5739-4486-9d05-687cfa48f5cd")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "MX_SW_HS"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "553f3b27-3656-4671-88d3-d0598444fb0f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "ee2e2bc8-1ff8-458f-9673-c6cdb4e7e27f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "119e6d97-c472-4eec-bc39-d83f289780ab")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted, Kailh CPG151101S11 for Cherry MX style switches"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "eb5e332c-e2c6-422f-ab15-2e706652bdc5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/b2c04ce7-32df-4a69-911b-8897471d4bf7")
		(sheetname "Stammblatt")
		(sheetfile "geebord-plate.kicad_sch")
		(attr exclude_from_pos_files allow_missing_courtyard)
		(fp_rect
			(start -9.525 -9.525)
			(end 9.525 9.525)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "Dwgs.User")
			(uuid "82bf902a-e946-4930-9229-352471337d1c")
		)
		(fp_line
			(start -7 -6.5)
			(end -7 6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "ae3eb2c5-0685-46c4-90d5-4b2582f7069e")
		)
		(fp_line
			(start -6.5 7)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "8805a638-3554-48df-bec6-209cb277dc72")
		)
		(fp_line
			(start 6.5 -7)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "53193ca4-d6d7-48fd-9356-4c01d082789c")
		)
		(fp_line
			(start 7 6.5)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "061b7bfd-b17e-4fd5-8ce5-cbafa6b0de13")
		)
		(fp_arc
			(start -7 -6.5)
			(mid -6.853553 -6.853553)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "2caa22af-b261-4638-85cb-00724b0fe1e3")
		)
		(fp_arc
			(start -6.497236 6.998884)
			(mid -6.850789 6.852437)
			(end -6.997236 6.498884)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "b7301a12-25b3-483c-80fd-4ad3b7784a7c")
		)
		(fp_arc
			(start 6.5 -7)
			(mid 6.853553 -6.853553)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "931e5bd8-9b85-444e-9749-f22aadb3f172")
		)
		(fp_arc
			(start 7 6.5)
			(mid 6.853553 6.853553)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "b7885024-28d0-4818-98e2-3e3c0d71d8bb")
		)
		(model "${KICAD8_3RD_PARTY}/3dmodels/com_github_perigoso_keyswitch-kicad-library/3d-library.3dshapes/SW_Cherry_MX_Plate.stp"
			(offset
				(xyz 0 0 -5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
		(layer "F.Cu")
		(uuid "1021d020-6e4a-424c-83b0-50c549ac4f91")
		(at 128.5875 80.9625)
		(property "Reference" "MX30"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
			(uuid "a3fc4f49-cdf9-493c-97c0-1d321685e38c")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "MX_SW_HS"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "182223f1-db1d-4eca-84aa-d25c9e7d2b1e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "abb4ee36-523b-4dfb-b782-b5dd113015d1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "cb87765d-ff11-4245-a151-a9a104c9dcc4")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted, Kailh CPG151101S11 for Cherry MX style switches"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "7bfb6e1b-a713-410d-b619-17bb9ab45270")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/7bb84b57-fbe8-4010-a8d5-653d29573335")
		(sheetname "Stammblatt")
		(sheetfile "geebord-plate.kicad_sch")
		(attr exclude_from_pos_files allow_missing_courtyard)
		(fp_rect
			(start -9.525 -9.525)
			(end 9.525 9.525)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "Dwgs.User")
			(uuid "2acadd35-25d3-47ba-b7f2-5908bfefc939")
		)
		(fp_line
			(start -7 -6.5)
			(end -7 6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "5ee1c703-fe39-42ee-acb5-669063d0fdb6")
		)
		(fp_line
			(start -6.5 7)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "49c65620-4a56-466c-a195-f12bb5305b88")
		)
		(fp_line
			(start 6.5 -7)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "80f2c4de-f94e-4520-9f84-ecb7e8f79648")
		)
		(fp_line
			(start 7 6.5)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "9dbe0cfa-3c93-46ea-8214-3d5b9842533a")
		)
		(fp_arc
			(start -7 -6.5)
			(mid -6.853553 -6.853553)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "164969b5-6aa6-4ca5-aac0-071f66975a86")
		)
		(fp_arc
			(start -6.497236 6.998884)
			(mid -6.850789 6.852437)
			(end -6.997236 6.498884)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "db833c21-c6c2-4bcd-ab9d-6cb04683f0a1")
		)
		(fp_arc
			(start 6.5 -7)
			(mid 6.853553 -6.853553)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "193b8e76-cd16-4d09-b17e-0087583f9183")
		)
		(fp_arc
			(start 7 6.5)
			(mid 6.853553 6.853553)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "e7419ec2-9f33-4291-816f-1f6323e1f59a")
		)
	)
	(footprint "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
		(layer "F.Cu")
		(uuid "10c5505c-e51d-422c-9e83-e5ccae961fae")
		(at 90.4875 42.8625)
		(property "Reference" "MX4"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
			(uuid "1b437f6d-ed70-4b93-b3a2-e6cda772d03b")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "MX_SW_HS"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "5f7d24f1-0792-4d1f-909d-291d84f9743a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "751119bc-3fab-437b-a28f-aba371382503")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "5dde00f9-e142-4485-8620-1e3d5fa7514b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted, Kailh CPG151101S11 for Cherry MX style switches"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "243e2b69-9bf2-48cd-a980-99a3529ec34c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/328cdcf0-afae-466c-9c79-76cba3315ef1")
		(sheetname "Stammblatt")
		(sheetfile "geebord-plate.kicad_sch")
		(attr exclude_from_pos_files allow_missing_courtyard)
		(fp_rect
			(start -9.525 -9.525)
			(end 9.525 9.525)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "Dwgs.User")
			(uuid "da63c3a9-912d-47c0-91ed-d029212de7aa")
		)
		(fp_line
			(start -7 -6.5)
			(end -7 6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "32ec9a86-cda2-4266-8d77-7921fb058850")
		)
		(fp_line
			(start -6.5 7)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "2ca5e1b2-6d4e-4f48-81f6-f19ec5298bcf")
		)
		(fp_line
			(start 6.5 -7)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "287af1b8-4bc5-48ba-8402-534b92be5abf")
		)
		(fp_line
			(start 7 6.5)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "2eb32f8a-5dbe-45c3-be8d-2db55b28dcaf")
		)
		(fp_arc
			(start -7 -6.5)
			(mid -6.853553 -6.853553)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "41f1b4aa-2ddd-4665-aca3-93169594914e")
		)
		(fp_arc
			(start -6.497236 6.998884)
			(mid -6.850789 6.852437)
			(end -6.997236 6.498884)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "a0652d1e-8fdf-4131-b910-0dffb157865e")
		)
		(fp_arc
			(start 6.5 -7)
			(mid 6.853553 -6.853553)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "3c1bbd50-5348-4255-95e4-aea838eec304")
		)
		(fp_arc
			(start 7 6.5)
			(mid 6.853553 6.853553)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "5a4bed94-cbea-4418-a7b8-de0781657088")
		)
	)
	(footprint "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
		(layer "F.Cu")
		(uuid "12194af5-a5c5-4a72-ac3b-245c6d465e04")
		(at 223.8375 42.8625)
		(property "Reference" "MX11"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
			(uuid "8a0d4476-accb-4a13-bd4d-12f0b11322c1")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "MX_SW_HS"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "c7c6fa70-9c3a-4cf6-bebf-bcffe7036a4d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "73e7f40b-7590-4847-91e2-425ec72aaefd")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "892fdc93-a7c8-4ac3-b18f-1d10ec3a6b65")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted, Kailh CPG151101S11 for Cherry MX style switches"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "0657cc1d-24e5-49df-854d-a476d8ae74e1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/81b7f801-83e5-40e1-b827-dac10865d872")
		(sheetname "Stammblatt")
		(sheetfile "geebord-plate.kicad_sch")
		(attr exclude_from_pos_files allow_missing_courtyard)
		(fp_rect
			(start -9.525 -9.525)
			(end 9.525 9.525)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "Dwgs.User")
			(uuid "33c722b6-b969-4ad1-90bf-5a7cd687f64f")
		)
		(fp_line
			(start -7 -6.5)
			(end -7 6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "be6f2641-5c0b-4c96-8f1b-256f9cde96ea")
		)
		(fp_line
			(start -6.5 7)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "033cbdb0-592b-4a98-9b80-a7b2d52f6585")
		)
		(fp_line
			(start 6.5 -7)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "1b72ea3d-73c7-48b3-adc0-a434c4128f89")
		)
		(fp_line
			(start 7 6.5)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "3087bb8f-101b-4fb1-a55b-d8db88249075")
		)
		(fp_arc
			(start -7 -6.5)
			(mid -6.853553 -6.853553)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "c743b3c1-eaeb-4155-9625-dc75ed73c7eb")
		)
		(fp_arc
			(start -6.497236 6.998884)
			(mid -6.850789 6.852437)
			(end -6.997236 6.498884)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "452c5da2-91c2-4a67-bd18-a5e0b2ea14af")
		)
		(fp_arc
			(start 6.5 -7)
			(mid 6.853553 -6.853553)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "80e9cc0c-85c8-416c-96f1-03f5d5be9ff0")
		)
		(fp_arc
			(start 7 6.5)
			(mid 6.853553 6.853553)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "e712bb50-ad7a-446b-92ea-7886c14bd242")
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad"
		(layer "F.Cu")
		(uuid "14c3ad8e-9934-4baa-9cf0-2d89db06f535")
		(at 20.1125 113.4375)
		(descr "Mounting Hole 3.2mm, M3, DIN965")
		(tags "mounting hole 3.2mm m3 din965")
		(property "Reference" "REF**"
			(at 0 -3.8 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "66dac61b-7f1c-4524-b98d-9534e4258cbd")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "MountingHole_3.2mm_M3_DIN965_Pad"
			(at 0 3.8 0)
			(layer "F.Fab")
			(uuid "5f04a0e2-6cf0-41ea-956a-3dd95955abac")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "757f949b-14d8-443c-95e9-3500290a5696")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "4e08b9f1-91e6-4112-9edb-008c87ae51f0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "f23ee5ca-a1c1-4d8e-9be0-b4f827d21e91")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_circle
			(center 0 0)
			(end 2.8 0)
			(stroke
				(width 0.15)
				(type solid)
			)
			(fill none)
			(layer "Cmts.User")
			(uuid "34ee176c-d882-4def-bf91-8fb6a663669c")
		)
		(fp_circle
			(center 0 0)
			(end 3.05 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill none)
			(layer "F.CrtYd")
			(uuid "f81813ac-92a0-4a2a-9312-6fd876e26bf4")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "df3f1b00-2b5c-4ec5-a783-367817bdb5c1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 5.6 5.6)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(uuid "4d66bacc-370f-425d-aac4-0466d5a716bc")
		)
	)
	(footprint "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
		(layer "F.Cu")
		(uuid "1d747894-c6e5-4fdb-a727-c30d4824a2a6")
		(at 223.8375 80.9625)
		(property "Reference" "MX35"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
			(uuid "4305e477-acce-4465-9a82-501f66a49719")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "MX_SW_HS"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "636e0f0a-64e7-4899-a948-553b5a514306")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "744e0358-beb5-4648-ba79-eecc1a050c27")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "099d00e1-70aa-44a5-b9fe-0e6dfe999265")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted, Kailh CPG151101S11 for Cherry MX style switches"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "4cf07521-6cfa-48fa-a98a-d875cdbc59ff")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/361c29c1-7e57-4409-b077-c415db5a20d8")
		(sheetname "Stammblatt")
		(sheetfile "geebord-plate.kicad_sch")
		(attr exclude_from_pos_files allow_missing_courtyard)
		(fp_rect
			(start -9.525 -9.525)
			(end 9.525 9.525)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "Dwgs.User")
			(uuid "6292a9bb-0cb8-462b-b2a9-cee92d59d3da")
		)
		(fp_line
			(start -7 -6.5)
			(end -7 6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "5d1f40ba-c4f0-4d40-8c19-6215133d77c4")
		)
		(fp_line
			(start -6.5 7)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "90d6971b-5849-442b-a606-f908dc54b672")
		)
		(fp_line
			(start 6.5 -7)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "673ee20f-1f81-44d8-a1ff-a9f5e86ad539")
		)
		(fp_line
			(start 7 6.5)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "5342aeff-82f6-47ba-8f5a-7fd99144c2f4")
		)
		(fp_arc
			(start -7 -6.5)
			(mid -6.853553 -6.853553)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "1da16a0f-e3d1-46a6-a7bf-e261a75d92c9")
		)
		(fp_arc
			(start -6.497236 6.998884)
			(mid -6.850789 6.852437)
			(end -6.997236 6.498884)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "85baa9d7-32e7-4df4-9303-3fe4efeb0a25")
		)
		(fp_arc
			(start 6.5 -7)
			(mid 6.853553 -6.853553)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "0535c735-5d12-44b7-9734-9a511f6fffbe")
		)
		(fp_arc
			(start 7 6.5)
			(mid 6.853553 6.853553)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "572c5c60-6fc8-4069-869c-d8749d374190")
		)
	)
	(footprint "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
		(layer "F.Cu")
		(uuid "26a794d4-91e4-4936-b322-c07b72bc611e")
		(at 109.5375 61.9125)
		(property "Reference" "MX17"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
			(uuid "436f8673-960d-4100-92c6-055e2e2f0cf7")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "MX_SW_HS"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "8d8f0b78-1298-415e-919b-79f4cad7ab28")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "6595717a-4bdb-4321-bee9-15f46992d747")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "04a97c00-b03a-4b49-a552-eb9da9746435")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted, Kailh CPG151101S11 for Cherry MX style switches"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "4b8b1fb5-26bd-46fa-a958-6ef8a978a193")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/cf832a05-bb6f-4c78-bee8-68656b2ce29e")
		(sheetname "Stammblatt")
		(sheetfile "geebord-plate.kicad_sch")
		(attr exclude_from_pos_files allow_missing_courtyard)
		(fp_rect
			(start -9.525 -9.525)
			(end 9.525 9.525)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "Dwgs.User")
			(uuid "ec2f4ff8-9998-4c2b-98d8-5a7d00491245")
		)
		(fp_line
			(start -7 -6.5)
			(end -7 6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "fa360b0b-855c-4d28-8d7a-d86f174f32a3")
		)
		(fp_line
			(start -6.5 7)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "73eb22d6-bc35-447c-a030-07bc0f953a28")
		)
		(fp_line
			(start 6.5 -7)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "fc707ece-7085-4380-adb8-e9d85ac2c3a1")
		)
		(fp_line
			(start 7 6.5)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "95427f2c-8af7-4f66-9f3e-fd5d1343d336")
		)
		(fp_arc
			(start -7 -6.5)
			(mid -6.853553 -6.853553)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "6e3cd977-0fda-4dd4-9fce-feb57e5db471")
		)
		(fp_arc
			(start -6.497236 6.998884)
			(mid -6.850789 6.852437)
			(end -6.997236 6.498884)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "65661456-cc25-4dfd-8ecc-807546a9e7dd")
		)
		(fp_arc
			(start 6.5 -7)
			(mid 6.853553 -6.853553)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "bcbf2cb2-e172-4960-9127-b18a2019bdc2")
		)
		(fp_arc
			(start 7 6.5)
			(mid 6.853553 6.853553)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "6913cc41-b6b7-4c83-99d0-3674d17e3ad9")
		)
	)
	(footprint "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
		(layer "F.Cu")
		(uuid "320a3d25-11b2-42c0-809b-ea7e5d048f23")
		(at 242.8875 80.9625)
		(property "Reference" "MX36"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
			(uuid "dd4671ed-a0d6-4c14-86d3-5ee66c6ad172")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "MX_SW_HS"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "9bed3021-c7eb-4c1e-a830-47dbd7a6f12e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "cb11c057-ab33-4cbb-8b71-49d5930b9a6b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "3d5a9fa7-5fe1-4f74-b6b2-4fae6f77874e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted, Kailh CPG151101S11 for Cherry MX style switches"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "eee42466-8f3e-4e86-a253-8393eaf9f738")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/bd2b7df4-4434-41b4-b2fb-76b7875ff750")
		(sheetname "Stammblatt")
		(sheetfile "geebord-plate.kicad_sch")
		(attr exclude_from_pos_files allow_missing_courtyard)
		(fp_rect
			(start -9.525 -9.525)
			(end 9.525 9.525)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "Dwgs.User")
			(uuid "ef7e8607-25e8-4d6c-8cef-376d37d99c45")
		)
		(fp_line
			(start -7 -6.5)
			(end -7 6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "404d0b43-c939-4464-837b-a431982744cf")
		)
		(fp_line
			(start -6.5 7)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "1e6820fa-4839-4ec9-9b57-d2dd6d3f94f8")
		)
		(fp_line
			(start 6.5 -7)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "a9defbeb-0349-4f3c-8032-49ab450f909b")
		)
		(fp_line
			(start 7 6.5)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "25346449-35b2-4636-b528-6c3343f66ef5")
		)
		(fp_arc
			(start -7 -6.5)
			(mid -6.853553 -6.853553)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "10510b41-7d29-4f5f-b03b-8d8072fd2c18")
		)
		(fp_arc
			(start -6.497236 6.998884)
			(mid -6.850789 6.852437)
			(end -6.997236 6.498884)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "d4cfb085-a1b8-425f-9f7b-4e72a6d4651f")
		)
		(fp_arc
			(start 6.5 -7)
			(mid 6.853553 -6.853553)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "5d1e5ac1-71b5-4648-ab6c-510dba805e89")
		)
		(fp_arc
			(start 7 6.5)
			(mid 6.853553 6.853553)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "d5a13634-0812-459c-9c20-0f47e21a8933")
		)
	)
	(footprint "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
		(layer "F.Cu")
		(uuid "34291d1f-db5e-4637-acc7-26eb1939dd70")
		(at 71.4375 42.8625)
		(property "Reference" "MX3"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
			(uuid "409da1cd-d8dd-4467-a26b-6018397f4314")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "MX_SW_HS"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "9b7913d2-03df-4360-a253-a54dcaa120eb")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "e0e1f533-c15a-4556-b828-0a8d6de17f99")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "f2b63180-5779-4e14-bdce-485ae3ee3fff")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted, Kailh CPG151101S11 for Cherry MX style switches"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "418f1787-d826-4965-82a0-d5bba37ed303")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/b9bd3d68-ff77-4da2-aa01-5447b1218d4a")
		(sheetname "Stammblatt")
		(sheetfile "geebord-plate.kicad_sch")
		(attr exclude_from_pos_files allow_missing_courtyard)
		(fp_rect
			(start -9.525 -9.525)
			(end 9.525 9.525)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "Dwgs.User")
			(uuid "8ae330e7-c39f-411a-9af6-6ad967d5ee24")
		)
		(fp_line
			(start -7 -6.5)
			(end -7 6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "f7dab206-9706-4766-b8f9-3441fda8c0fa")
		)
		(fp_line
			(start -6.5 7)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "f9f727cc-68e9-4ed3-b119-4ff1096bf229")
		)
		(fp_line
			(start 6.5 -7)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "614d2071-ba53-499c-87f8-f4c3ded857b5")
		)
		(fp_line
			(start 7 6.5)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "75d0a33d-1b88-4bf9-b3cd-9b16b71e5615")
		)
		(fp_arc
			(start -7 -6.5)
			(mid -6.853553 -6.853553)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "fe3e58e7-e524-4ff5-8cc4-196e35f94032")
		)
		(fp_arc
			(start -6.497236 6.998884)
			(mid -6.850789 6.852437)
			(end -6.997236 6.498884)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "0194c440-0248-4a1a-8f25-0250e08f2966")
		)
		(fp_arc
			(start 6.5 -7)
			(mid 6.853553 -6.853553)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "cfa5a8fe-73df-4647-bc05-13a558762733")
		)
		(fp_arc
			(start 7 6.5)
			(mid 6.853553 6.853553)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "e1f66177-ff25-4589-b07c-9fe44d9f753a")
		)
	)
	(footprint "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
		(layer "F.Cu")
		(uuid "35942029-a285-490d-8595-a5d72ff277be")
		(at 71.4375 100.0125)
		(property "Reference" "MX39"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
			(uuid "f2264b72-b255-4da9-8980-f670534c2b67")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "MX_SW_HS"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "fb0dafc5-3498-452d-9086-867c8f6a9832")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "15d1453a-0119-4fc4-abe8-0cd1f594decc")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "25500574-f9f5-45fa-a814-52cdfedba7a9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted, Kailh CPG151101S11 for Cherry MX style switches"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "35499a29-b0a9-4c58-83c6-748946bb5c72")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/0836c125-ec2c-41c9-a093-3ab140927ce6")
		(sheetname "Stammblatt")
		(sheetfile "geebord-plate.kicad_sch")
		(attr exclude_from_pos_files allow_missing_courtyard)
		(fp_rect
			(start -9.525 -9.525)
			(end 9.525 9.525)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "Dwgs.User")
			(uuid "35d7bc54-ca12-472a-b54d-d362308b78f0")
		)
		(fp_line
			(start -7 -6.5)
			(end -7 6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "cf83d828-ae4b-4e6c-a8dd-37896c28671a")
		)
		(fp_line
			(start -6.5 7)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "f55c74d4-d4e8-480a-8892-4e8695756313")
		)
		(fp_line
			(start 6.5 -7)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "324eb536-43a9-41df-95a8-63af3f7ef331")
		)
		(fp_line
			(start 7 6.5)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "88445e41-e6fc-458d-bb97-888aed2e8dc5")
		)
		(fp_arc
			(start -7 -6.5)
			(mid -6.853553 -6.853553)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "3b092c6b-866f-488c-adef-de0a04f290c3")
		)
		(fp_arc
			(start -6.497236 6.998884)
			(mid -6.850789 6.852437)
			(end -6.997236 6.498884)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "17be0c22-41bb-43d3-a580-a2c52367212b")
		)
		(fp_arc
			(start 6.5 -7)
			(mid 6.853553 -6.853553)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "c2ded841-de75-4ffb-b261-88296f99a4a9")
		)
		(fp_arc
			(start 7 6.5)
			(mid 6.853553 6.853553)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "2f8fb13f-298a-4b68-ac8f-e256136f5722")
		)
	)
	(footprint "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
		(layer "F.Cu")
		(uuid "43fadd77-1387-4c9b-81bb-f85fb217e10c")
		(at 204.7875 61.9125)
		(property "Reference" "MX22"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
			(uuid "88a83e84-42ad-4423-b7af-45955bf9c2c2")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "MX_SW_HS"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "4cff5ee1-15fa-4aa1-86bd-f9e11a5bf396")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "fad19e1d-abb8-42de-abe5-097163fc2694")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "65839362-1251-4022-9b53-cda0a918bed9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted, Kailh CPG151101S11 for Cherry MX style switches"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "5e685c10-830f-47a5-955d-edb29839b2cf")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/7332fccb-abd1-4568-88d7-97e53e825263")
		(sheetname "Stammblatt")
		(sheetfile "geebord-plate.kicad_sch")
		(attr exclude_from_pos_files allow_missing_courtyard)
		(fp_rect
			(start -9.525 -9.525)
			(end 9.525 9.525)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "Dwgs.User")
			(uuid "d1b2ba36-4d82-46ce-804b-cc85a9f1a6bf")
		)
		(fp_line
			(start -7 -6.5)
			(end -7 6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "5c91bab9-006a-4cc6-901b-367759f2b739")
		)
		(fp_line
			(start -6.5 7)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "879b642e-9d73-43bc-b910-c719ae06785e")
		)
		(fp_line
			(start 6.5 -7)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "9d7cf47f-43bf-48ab-a870-36a9856093d8")
		)
		(fp_line
			(start 7 6.5)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "df2ea092-008a-4ba3-87fb-47d5092a423e")
		)
		(fp_arc
			(start -7 -6.5)
			(mid -6.853553 -6.853553)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "fa4286b3-a3a8-4fc9-88b2-78eb09d18f56")
		)
		(fp_arc
			(start -6.497236 6.998884)
			(mid -6.850789 6.852437)
			(end -6.997236 6.498884)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "8d206856-f6e0-4272-82c0-97d049b58a99")
		)
		(fp_arc
			(start 6.5 -7)
			(mid 6.853553 -6.853553)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "8aa9ea53-fc0f-4014-997c-e0bb451baadf")
		)
		(fp_arc
			(start 7 6.5)
			(mid 6.853553 6.853553)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "9c7a7034-59ba-4490-b8f7-655d5b911713")
		)
	)
	(footprint "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
		(layer "F.Cu")
		(uuid "44d5fb79-3113-4380-be52-ab4b2e45cd21")
		(at 109.5375 42.8625)
		(property "Reference" "MX5"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
			(uuid "e36af3e2-2497-45b9-8069-407c5369aef5")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "MX_SW_HS"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "767b3311-ff28-40f9-bc75-17699a24583a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "cf0bc585-f7bc-4001-a059-0b1ccf8d0111")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "5a2e9cd3-b2ba-4c3f-ae77-dacc4a82c7ff")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted, Kailh CPG151101S11 for Cherry MX style switches"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "21874ef9-d771-4689-9ca4-0cc48271d8bd")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/df0d56de-545d-496f-85b4-737cf1caa2c8")
		(sheetname "Stammblatt")
		(sheetfile "geebord-plate.kicad_sch")
		(attr exclude_from_pos_files allow_missing_courtyard)
		(fp_rect
			(start -9.525 -9.525)
			(end 9.525 9.525)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "Dwgs.User")
			(uuid "28de0db9-8844-48d7-b2c8-7f8bb1ffbede")
		)
		(fp_line
			(start -7 -6.5)
			(end -7 6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "080afae7-b7be-4c29-b953-495284eb6173")
		)
		(fp_line
			(start -6.5 7)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "34d45b58-4cbb-4745-8d32-1d65ef961814")
		)
		(fp_line
			(start 6.5 -7)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "778bc418-ed2f-40c2-a2b5-6541fb553733")
		)
		(fp_line
			(start 7 6.5)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "5c467328-d8d9-439a-97d5-bdcc083274d5")
		)
		(fp_arc
			(start -7 -6.5)
			(mid -6.853553 -6.853553)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "2328b4da-3477-4323-8e03-83ff9f2dca82")
		)
		(fp_arc
			(start -6.497236 6.998884)
			(mid -6.850789 6.852437)
			(end -6.997236 6.498884)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "64cb6094-4cb7-4563-bb5d-69d6d2d4ab24")
		)
		(fp_arc
			(start 6.5 -7)
			(mid 6.853553 -6.853553)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "2f830eb6-fefc-4428-a98b-eb39d4c77ac4")
		)
		(fp_arc
			(start 7 6.5)
			(mid 6.853553 6.853553)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "8111f74f-398b-4997-a678-7caeeede3956")
		)
	)
	(footprint "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
		(layer "F.Cu")
		(uuid "4e454922-dc83-4e43-a4be-bbbcb07d39d4")
		(at 71.4375 80.9625)
		(property "Reference" "MX27"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
			(uuid "649462e5-f799-4251-a522-0975ed38f35f")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "MX_SW_HS"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "c19319e7-1506-4ce1-8d7f-d74eedf7159c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "c522da85-48db-45a4-a31b-1b49142792cf")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "9a775ead-a687-4c64-bb30-62d316b0d702")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted, Kailh CPG151101S11 for Cherry MX style switches"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "7550202b-6b9f-43ed-a87b-c1d6ee17538e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/d0dc0423-bb41-4b85-b488-6ac4882a368a")
		(sheetname "Stammblatt")
		(sheetfile "geebord-plate.kicad_sch")
		(attr exclude_from_pos_files allow_missing_courtyard)
		(fp_rect
			(start -9.525 -9.525)
			(end 9.525 9.525)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "Dwgs.User")
			(uuid "dcce8154-a0ed-4a12-a087-2fa376bacbf9")
		)
		(fp_line
			(start -7 -6.5)
			(end -7 6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "b79431a4-2164-4635-9a27-f7bc956cb02b")
		)
		(fp_line
			(start -6.5 7)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "5f77c84f-2f66-4e14-ad12-d18296e51f6c")
		)
		(fp_line
			(start 6.5 -7)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "b8ed1be2-924f-4f5f-87bb-003d39f7bfc3")
		)
		(fp_line
			(start 7 6.5)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "79b9031b-e5b5-4974-a341-452c6a728631")
		)
		(fp_arc
			(start -7 -6.5)
			(mid -6.853553 -6.853553)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "7ad66b27-a247-4eee-a9e8-5880c67efebf")
		)
		(fp_arc
			(start -6.497236 6.998884)
			(mid -6.850789 6.852437)
			(end -6.997236 6.498884)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "4b8249d9-6b6c-471d-8cb3-a21ba9a5c969")
		)
		(fp_arc
			(start 6.5 -7)
			(mid 6.853553 -6.853553)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "3277c6e0-0f8f-434b-9a48-41f8ac9d4232")
		)
		(fp_arc
			(start 7 6.5)
			(mid 6.853553 6.853553)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "b116ca07-f45a-4206-b0c4-166f8e58c03e")
		)
	)
	(footprint "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
		(layer "F.Cu")
		(uuid "57332a5c-0c35-44bc-88a3-e6540e78f1cc")
		(at 185.7375 100.0125)
		(property "Reference" "MX43"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
			(uuid "ddf2fdd5-c5e0-4ccd-864a-6aa67f7907f2")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "MX_SW_HS"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "ca74512b-51fc-4701-a128-31daf115d43f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "884a92e1-dd67-456f-a1fe-0b8fc126e47b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "f63cbe5c-fb15-4d3e-b859-5f0e992a7c31")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted, Kailh CPG151101S11 for Cherry MX style switches"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "d2149b3a-2ba4-458d-9f1c-4da29a27dc69")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/21985cfd-0448-4504-9ed7-0434378ee190")
		(sheetname "Stammblatt")
		(sheetfile "geebord-plate.kicad_sch")
		(attr exclude_from_pos_files allow_missing_courtyard)
		(fp_rect
			(start -9.525 -9.525)
			(end 9.525 9.525)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "Dwgs.User")
			(uuid "491d2e7c-98fb-48b1-bf7c-309dfc58b4cc")
		)
		(fp_line
			(start -7 -6.5)
			(end -7 6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "056389db-a3e4-4a72-bb14-f0f70d401bb0")
		)
		(fp_line
			(start -6.5 7)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "51639fb6-887a-4b7b-90ee-6fafa5a22ad4")
		)
		(fp_line
			(start 6.5 -7)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "28d196ff-f565-4225-8a0e-0bfa40f374ea")
		)
		(fp_line
			(start 7 6.5)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "c45f5060-588f-4315-868d-1f65b81aa6d9")
		)
		(fp_arc
			(start -7 -6.5)
			(mid -6.853553 -6.853553)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "ff581897-1a9f-4557-9752-6fb3b33295ff")
		)
		(fp_arc
			(start -6.497236 6.998884)
			(mid -6.850789 6.852437)
			(end -6.997236 6.498884)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "b8fe2968-4dd3-494c-a7b4-fed677b35969")
		)
		(fp_arc
			(start 6.5 -7)
			(mid 6.853553 -6.853553)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "354f04c2-7a0a-468b-bf18-37c832072cb3")
		)
		(fp_arc
			(start 7 6.5)
			(mid 6.853553 6.853553)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "f110aba8-9ada-4bc4-9ca4-7d758b99c11e")
		)
	)
	(footprint "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
		(layer "F.Cu")
		(uuid "6d15548a-b95f-4547-991e-824977a683a1")
		(at 204.7875 80.9625)
		(property "Reference" "MX34"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
			(uuid "be5e5d3e-967e-452c-a14a-1c746ba77609")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "MX_SW_HS"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "4fd84c9f-9946-4792-8597-b36fc9af1b25")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "660fd63d-c0b8-431d-8bb9-6cd7e355b147")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "8169e485-e3fe-4b19-8a63-9064889242fa")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted, Kailh CPG151101S11 for Cherry MX style switches"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "0b978112-5f0f-4b26-b204-c866b04f0d26")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/15465e9e-e6e7-4475-aaca-cb88fcfd1694")
		(sheetname "Stammblatt")
		(sheetfile "geebord-plate.kicad_sch")
		(attr exclude_from_pos_files allow_missing_courtyard)
		(fp_rect
			(start -9.525 -9.525)
			(end 9.525 9.525)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "Dwgs.User")
			(uuid "1e0865d9-8451-4439-adb1-5f1acf9b5185")
		)
		(fp_line
			(start -7 -6.5)
			(end -7 6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "3b62df4b-29c7-4f0c-a7cf-a9b0bfd3cad6")
		)
		(fp_line
			(start -6.5 7)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "25073a81-4d61-408d-91f0-8122b95e990b")
		)
		(fp_line
			(start 6.5 -7)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "3c10c2cc-29e9-4f32-b90c-561eed382068")
		)
		(fp_line
			(start 7 6.5)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "bc4ec148-9ac3-4b34-b014-dfb753c0c372")
		)
		(fp_arc
			(start -7 -6.5)
			(mid -6.853553 -6.853553)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "1d3b5746-4898-4e07-859e-fe528e352496")
		)
		(fp_arc
			(start -6.497236 6.998884)
			(mid -6.850789 6.852437)
			(end -6.997236 6.498884)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "4618e87e-81ae-4832-a380-c2524355aef0")
		)
		(fp_arc
			(start 6.5 -7)
			(mid 6.853553 -6.853553)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "eee0e357-89b6-42ca-9056-f41b18f94104")
		)
		(fp_arc
			(start 7 6.5)
			(mid 6.853553 6.853553)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "9779f29f-d3a5-4b7a-b8ed-35c1a33dbbe1")
		)
	)
	(footprint "PCM_marbastlib-xp-plate-mx:Plate_MX_1.5u"
		(layer "F.Cu")
		(uuid "6e508d9a-2c2c-4210-b3ba-98bb8da071f4")
		(at 161.925 100.0125)
		(property "Reference" "MX42"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
			(uuid "26cfe31a-fe3e-4e69-b4be-b1e955ec3e2f")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "MX_SW_HS"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "2f03fa27-0614-4159-afda-cf6a987a962f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "PCM_marbastlib-xp-plate-mx:Plate_MX_1.5u"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "00fa3e17-86d8-4c41-9660-6a5895778577")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "31112496-8f12-4ff5-8cc0-92d5c88c0acc")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted, Kailh CPG151101S11 for Cherry MX style switches"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "9699ed77-50f6-4ba9-a0df-269e9bdcabb5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/c0a2cfd4-7342-4581-920a-dc876a32c3b0")
		(sheetname "Stammblatt")
		(sheetfile "geebord-plate.kicad_sch")
		(attr exclude_from_pos_files allow_missing_courtyard)
		(fp_rect
			(start -14.2875 -9.525)
			(end 14.2875 9.525)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "Dwgs.User")
			(uuid "724ee618-d036-452b-b565-1aacb581d41f")
		)
		(fp_line
			(start -7 -6.5)
			(end -7 6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "8f71132b-8e39-4217-b407-d3effc4257fe")
		)
		(fp_line
			(start -6.5 7)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "5f8c93ec-4a35-4107-b020-eadbb16b512b")
		)
		(fp_line
			(start 6.5 -7)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "17d27a0b-dbb5-4ced-96b1-a5443257bfdd")
		)
		(fp_line
			(start 7 6.5)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "dcaa9c8f-c537-4c39-aa6f-30895e4674f0")
		)
		(fp_arc
			(start -7 -6.5)
			(mid -6.853553 -6.853553)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "cc2d0838-2e28-43bf-bbad-e923886d9a2f")
		)
		(fp_arc
			(start -6.497236 6.998884)
			(mid -6.850789 6.852437)
			(end -6.997236 6.498884)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "875d909e-cefe-4420-b3a1-3747ad9e5378")
		)
		(fp_arc
			(start 6.5 -7)
			(mid 6.853553 -6.853553)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "99bb9d0f-bf9d-4c49-af87-590fde2e34bf")
		)
		(fp_arc
			(start 7 6.5)
			(mid 6.853553 6.853553)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "4ef024c0-2da9-4b74-8975-8ea2a2ca735c")
		)
	)
	(footprint "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
		(layer "F.Cu")
		(uuid "767ee0a4-b17f-429b-a03c-d98e6d0be083")
		(at 242.8875 42.8625)
		(property "Reference" "MX12"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
			(uuid "b9da1a80-183d-4b3d-a2be-99e62e5f0882")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "MX_SW_HS"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "2e51fe13-1d87-41bf-957a-f86a61a27507")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "a7078dac-84f4-44d7-8772-7187d4934a3f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "d69d7a9f-b59c-438d-aa59-6371e780e00f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted, Kailh CPG151101S11 for Cherry MX style switches"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "0ec26c3f-758d-4a38-ac2c-98e80428ed65")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/11ddac2d-6d6d-4a0c-8932-c18f28f0acdd")
		(sheetname "Stammblatt")
		(sheetfile "geebord-plate.kicad_sch")
		(attr exclude_from_pos_files allow_missing_courtyard)
		(fp_rect
			(start -9.525 -9.525)
			(end 9.525 9.525)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "Dwgs.User")
			(uuid "f30720c4-8ca7-4f31-84bb-fa6ebecfe9cb")
		)
		(fp_line
			(start -7 -6.5)
			(end -7 6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "d5b10aa5-f10b-42d7-b62b-b5098e140151")
		)
		(fp_line
			(start -6.5 7)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "ce7763e6-10db-48f9-a53b-3ce01f09c639")
		)
		(fp_line
			(start 6.5 -7)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "f63088a3-7ea3-44da-b1ab-c327d6213cac")
		)
		(fp_line
			(start 7 6.5)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "291fc320-57f5-45c5-8b23-b10493ca478e")
		)
		(fp_arc
			(start -7 -6.5)
			(mid -6.853553 -6.853553)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "9234f3f9-3e96-46e9-9a00-95124966126b")
		)
		(fp_arc
			(start -6.497236 6.998884)
			(mid -6.850789 6.852437)
			(end -6.997236 6.498884)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "077c49e4-6b9c-4580-b8b9-04afb2212817")
		)
		(fp_arc
			(start 6.5 -7)
			(mid 6.853553 -6.853553)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "8a5288bf-2796-4fd7-a27a-5d40cced32dd")
		)
		(fp_arc
			(start 7 6.5)
			(mid 6.853553 6.853553)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "b497bfe9-c76c-4766-8a44-fe6db773becc")
		)
		(model "${KICAD8_3RD_PARTY}/3dmodels/com_github_perigoso_keyswitch-kicad-library/3d-library.3dshapes/SW_Cherry_MX_Plate.stp"
			(offset
				(xyz 0 0 -5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
		(layer "F.Cu")
		(uuid "78445f28-70d6-4f29-b7b2-c212936b33e0")
		(at 90.4875 61.9125)
		(property "Reference" "MX16"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
			(uuid "84116e6f-106e-4fd8-ae20-b2b9d5032731")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "MX_SW_HS"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "57dc85f1-8f6c-44fc-b1a3-9a802d34f609")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "a7156ae4-e2f0-4b3b-ae6b-cf4cf081bb0f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "9f11b8b3-ef9e-4cc5-b1b6-0612b3166db8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted, Kailh CPG151101S11 for Cherry MX style switches"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "30e5bf4d-7ab9-4cf3-b361-7def78a397c7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/9b690ba9-32fb-44e3-83a6-e15c452e5478")
		(sheetname "Stammblatt")
		(sheetfile "geebord-plate.kicad_sch")
		(attr exclude_from_pos_files allow_missing_courtyard)
		(fp_rect
			(start -9.525 -9.525)
			(end 9.525 9.525)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "Dwgs.User")
			(uuid "82ad5aa5-74f7-4d1f-90c8-677fc867101c")
		)
		(fp_line
			(start -7 -6.5)
			(end -7 6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "faba853b-cfdf-4bc0-8be4-4c854263e14c")
		)
		(fp_line
			(start -6.5 7)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "840bb403-6259-47dd-b978-ee6ef6fae105")
		)
		(fp_line
			(start 6.5 -7)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "444e47a2-dfde-4848-a972-899f7d207992")
		)
		(fp_line
			(start 7 6.5)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "47fce286-16a1-4b44-8bb7-f53c44cf93f6")
		)
		(fp_arc
			(start -7 -6.5)
			(mid -6.853553 -6.853553)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "8fa486bc-6e97-440a-94e3-73889909b9f8")
		)
		(fp_arc
			(start -6.497236 6.998884)
			(mid -6.850789 6.852437)
			(end -6.997236 6.498884)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "1ebe2c1d-476c-4f96-894f-f272c29f4f4c")
		)
		(fp_arc
			(start 6.5 -7)
			(mid 6.853553 -6.853553)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "cf28d8e4-71cf-49d6-b91d-d19efd3b4833")
		)
		(fp_arc
			(start 7 6.5)
			(mid 6.853553 6.853553)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "1a5dc317-721c-4166-9fc7-f8c10e12c280")
		)
	)
	(footprint "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
		(layer "F.Cu")
		(uuid "7a6764b9-be56-45ab-accd-e9a288286083")
		(at 166.6875 80.9625)
		(property "Reference" "MX32"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
			(uuid "a792c74d-bea0-417b-a8ae-87ecdbd3c800")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "MX_SW_HS"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "bf16d4b8-d33c-4a40-a326-3d5d506d8f05")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "8c74aa66-89a2-47c1-adeb-c15d3d4cd228")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "40db6e85-6516-4f35-b6ea-538c17fcab0d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted, Kailh CPG151101S11 for Cherry MX style switches"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "11b67e6f-51d8-420c-b7f2-d85796537c7a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/dbf083e3-1686-42d2-a1d5-5ce017beadd4")
		(sheetname "Stammblatt")
		(sheetfile "geebord-plate.kicad_sch")
		(attr exclude_from_pos_files allow_missing_courtyard)
		(fp_rect
			(start -9.525 -9.525)
			(end 9.525 9.525)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "Dwgs.User")
			(uuid "52c9415c-fa3a-4098-b73d-743224337924")
		)
		(fp_line
			(start -7 -6.5)
			(end -7 6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "697431c7-56a0-46f1-b735-9797f7df6cc1")
		)
		(fp_line
			(start -6.5 7)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "62d84fbf-5246-499a-9526-3e3c1b7590f0")
		)
		(fp_line
			(start 6.5 -7)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "62309265-48e2-4941-a230-02c1a275c02c")
		)
		(fp_line
			(start 7 6.5)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "b4865154-71e0-4420-a079-4a13a1c16911")
		)
		(fp_arc
			(start -7 -6.5)
			(mid -6.853553 -6.853553)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "bfacb9a3-ca4e-4939-83d6-7bfcf9f0b02b")
		)
		(fp_arc
			(start -6.497236 6.998884)
			(mid -6.850789 6.852437)
			(end -6.997236 6.498884)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "dd4781c7-3b55-4a6a-b9f8-bc575e1611d3")
		)
		(fp_arc
			(start 6.5 -7)
			(mid 6.853553 -6.853553)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "99d8ab94-3825-4e15-b619-fbf63cacd6fd")
		)
		(fp_arc
			(start 7 6.5)
			(mid 6.853553 6.853553)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "2706742d-f863-4e9d-8334-df10d4c9a808")
		)
	)
	(footprint "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
		(layer "F.Cu")
		(uuid "7b5cac1f-96c9-47ca-b78a-52f3eb36d842")
		(at 166.6875 61.9125)
		(property "Reference" "MX20"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
			(uuid "818c7f31-9be7-432f-9237-069b8587be4a")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "MX_SW_HS"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "3e9aa15f-c178-4d21-aef3-e731c00e9707")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "302b76d1-0dc9-46a9-b133-74b9a691f7fb")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "bcf587f1-0da5-4ee7-b146-e010287982fe")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted, Kailh CPG151101S11 for Cherry MX style switches"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "2697cd77-3385-47d3-a3f2-87edbed8adab")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/7cf32ff5-5a11-4bc7-a810-dcb20f37000e")
		(sheetname "Stammblatt")
		(sheetfile "geebord-plate.kicad_sch")
		(attr exclude_from_pos_files allow_missing_courtyard)
		(fp_rect
			(start -9.525 -9.525)
			(end 9.525 9.525)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "Dwgs.User")
			(uuid "51200727-d4cf-463f-95c3-457627ba434c")
		)
		(fp_line
			(start -7 -6.5)
			(end -7 6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "4aa552d7-7f79-4fcc-a241-c1ee5d6efadd")
		)
		(fp_line
			(start -6.5 7)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "6506deb7-47a4-40bb-8a1d-b111725bda6e")
		)
		(fp_line
			(start 6.5 -7)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "2f1a42ad-a4fd-4b27-a858-77c3f37e112c")
		)
		(fp_line
			(start 7 6.5)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "286561fe-13f9-4220-93b9-16f3da48e2fd")
		)
		(fp_arc
			(start -7 -6.5)
			(mid -6.853553 -6.853553)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "ce506d9e-80b1-4de1-bef9-d810baca4409")
		)
		(fp_arc
			(start -6.497236 6.998884)
			(mid -6.850789 6.852437)
			(end -6.997236 6.498884)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "31e5d74c-6b75-413a-85bf-8ce516be02ef")
		)
		(fp_arc
			(start 6.5 -7)
			(mid 6.853553 -6.853553)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "36e34a82-94df-49ec-9a1c-59a04dd3f411")
		)
		(fp_arc
			(start 7 6.5)
			(mid 6.853553 6.853553)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "3cdc78f3-f725-445e-9d9e-2e4ac502f401")
		)
	)
	(footprint "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
		(layer "F.Cu")
		(uuid "7bd14aa6-e7cc-44e3-b0f1-03923316c496")
		(at 147.6375 61.9125)
		(property "Reference" "MX19"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
			(uuid "00191563-c8d4-42d6-8a05-2c83993c2b8d")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "MX_SW_HS"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "7cd2b550-b334-4802-a177-508b2922c739")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "eccdae52-0515-4393-aab1-b897ae959a9b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "661e83d6-e4c6-4250-bd07-c9526bcc7e4f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted, Kailh CPG151101S11 for Cherry MX style switches"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "af98b5df-fec8-47c3-878f-97129c73baa6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/bfbc4d09-f793-40ce-95a4-e20dedd0db4b")
		(sheetname "Stammblatt")
		(sheetfile "geebord-plate.kicad_sch")
		(attr exclude_from_pos_files allow_missing_courtyard)
		(fp_rect
			(start -9.525 -9.525)
			(end 9.525 9.525)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "Dwgs.User")
			(uuid "f3b51273-5c77-4abb-a34d-afaf24070433")
		)
		(fp_line
			(start -7 -6.5)
			(end -7 6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "3326ec25-61db-4e68-bb59-c163dc69b21b")
		)
		(fp_line
			(start -6.5 7)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "351778a4-b99a-42f8-9bf1-580044def3cf")
		)
		(fp_line
			(start 6.5 -7)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "542e857c-d930-44b9-a44b-0a66f7bf7b9e")
		)
		(fp_line
			(start 7 6.5)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "1341987d-a36b-495c-bccb-42b2c9c20d92")
		)
		(fp_arc
			(start -7 -6.5)
			(mid -6.853553 -6.853553)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "be1a1280-860f-4725-be24-2b1f3ceb4503")
		)
		(fp_arc
			(start -6.497236 6.998884)
			(mid -6.850789 6.852437)
			(end -6.997236 6.498884)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "c093f4c5-276c-4965-8bb6-3c47a2e4e980")
		)
		(fp_arc
			(start 6.5 -7)
			(mid 6.853553 -6.853553)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "c03e739c-24dc-4e00-97c9-b3ee65ed7a1e")
		)
		(fp_arc
			(start 7 6.5)
			(mid 6.853553 6.853553)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "ff003797-df82-4b7b-b150-067138f4043e")
		)
	)
	(footprint "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
		(layer "F.Cu")
		(uuid "7e8abd57-20ac-4f3a-a372-97e1547f38f2")
		(at 185.7375 80.9625)
		(property "Reference" "MX33"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
			(uuid "b2ae25b0-b79b-45f1-a36a-0daa46062192")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "MX_SW_HS"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "e9a7eb01-e51e-44c5-9253-a9045a80fcb4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "7e87da60-3a5f-4448-8adc-0cba73b0171f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "bfec7b91-fbf9-4222-b544-99151640a127")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted, Kailh CPG151101S11 for Cherry MX style switches"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "466ba1f5-4d96-42d4-8b4d-8fdcc60a92fb")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/d0fd0468-0d34-4fa4-8093-38a4a4a86b12")
		(sheetname "Stammblatt")
		(sheetfile "geebord-plate.kicad_sch")
		(attr exclude_from_pos_files allow_missing_courtyard)
		(fp_rect
			(start -9.525 -9.525)
			(end 9.525 9.525)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "Dwgs.User")
			(uuid "15941769-90a1-46cb-b6ef-90e56337fe12")
		)
		(fp_line
			(start -7 -6.5)
			(end -7 6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "84f8cefa-e1ad-4912-9162-c028117866db")
		)
		(fp_line
			(start -6.5 7)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "45ed1b47-7465-4345-b4f0-e1706513a629")
		)
		(fp_line
			(start 6.5 -7)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "631e543d-8550-49ca-a337-7485229bfda3")
		)
		(fp_line
			(start 7 6.5)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "a47f128e-9949-4c40-8b90-dbce36223e81")
		)
		(fp_arc
			(start -7 -6.5)
			(mid -6.853553 -6.853553)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "2bfd39e6-4872-4126-a5fc-fc438e4e7dc2")
		)
		(fp_arc
			(start -6.497236 6.998884)
			(mid -6.850789 6.852437)
			(end -6.997236 6.498884)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "a7be2412-b175-461d-a365-4cae6737c4f7")
		)
		(fp_arc
			(start 6.5 -7)
			(mid 6.853553 -6.853553)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "e7c0e2d8-3cb1-49ea-ac80-976adc4d029b")
		)
		(fp_arc
			(start 7 6.5)
			(mid 6.853553 6.853553)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "74772a23-c8e9-4e23-a1ce-1d82bde3375f")
		)
	)
	(footprint "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
		(layer "F.Cu")
		(uuid "7f29ad66-2c3f-41d9-8986-133e05adfd6b")
		(at 128.5875 61.9125)
		(property "Reference" "MX18"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
			(uuid "19ded841-d00c-4136-a089-397f3a207886")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "MX_SW_HS"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "b997a057-32d3-4258-9957-d80b0a4f94f9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "cb54efbc-db44-4dec-accb-480bb5d881fe")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "74c3a5a1-cd5d-4473-acae-98f9042d8004")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted, Kailh CPG151101S11 for Cherry MX style switches"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "83386728-41ee-46da-a942-f95e199cefb4")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/f29fc2cc-04cd-4dd3-a62f-bd023af5c074")
		(sheetname "Stammblatt")
		(sheetfile "geebord-plate.kicad_sch")
		(attr exclude_from_pos_files allow_missing_courtyard)
		(fp_rect
			(start -9.525 -9.525)
			(end 9.525 9.525)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "Dwgs.User")
			(uuid "1dabfc7e-54b3-45ca-99e7-580de36af02d")
		)
		(fp_line
			(start -7 -6.5)
			(end -7 6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "233cd215-3d89-4875-b257-7a3f2dade1ac")
		)
		(fp_line
			(start -6.5 7)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "632333b1-8eb9-4325-848b-7896607ae657")
		)
		(fp_line
			(start 6.5 -7)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "bbc2b633-94a3-4cf3-829b-f39555323e61")
		)
		(fp_line
			(start 7 6.5)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "2df82669-e7eb-403c-a550-4efd1e83677a")
		)
		(fp_arc
			(start -7 -6.5)
			(mid -6.853553 -6.853553)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "f140c0ac-dd74-4041-901d-ee3648cb78fc")
		)
		(fp_arc
			(start -6.497236 6.998884)
			(mid -6.850789 6.852437)
			(end -6.997236 6.498884)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "fdfee231-3243-43c1-95ec-3eeedba54243")
		)
		(fp_arc
			(start 6.5 -7)
			(mid 6.853553 -6.853553)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "2bcf4faa-48b2-46ef-902c-2f16f7f415aa")
		)
		(fp_arc
			(start 7 6.5)
			(mid 6.853553 6.853553)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "32aa3377-1135-45e2-94d2-431bf4c09bb2")
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad"
		(layer "F.Cu")
		(uuid "808a5fc2-24f7-49c9-b720-2a501d97acbf")
		(at 20.1125 29.4375)
		(descr "Mounting Hole 3.2mm, M3, DIN965")
		(tags "mounting hole 3.2mm m3 din965")
		(property "Reference" "REF**"
			(at 6.367 -0.037 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "243dff29-3afc-4648-a55d-b72ec1825ab1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "MountingHole_3.2mm_M3_DIN965_Pad"
			(at 0 3.8 0)
			(layer "F.Fab")
			(uuid "09525d1b-9f95-422b-8fe6-a00f8d9813b6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "7daa065d-fed5-4709-ab10-3cabef53f2cb")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "37d86404-f96e-464c-9962-bd0d859d5bd4")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "2e3aae25-c2a9-4c4b-9aca-5e9192eaa84b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_circle
			(center 0 0)
			(end 2.8 0)
			(stroke
				(width 0.15)
				(type solid)
			)
			(fill none)
			(layer "Cmts.User")
			(uuid "fce5d06d-3448-479a-9f5d-31c49829ad8e")
		)
		(fp_circle
			(center 0 0)
			(end 3.05 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill none)
			(layer "F.CrtYd")
			(uuid "f9078249-e3af-4402-b5ae-dc560b4f12e3")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "d81857f0-702e-4ec3-9d4b-47ebc911ce5a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 5.6 5.6)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(uuid "59f163b5-6f70-4a41-a25b-2c11e851d6b3")
		)
	)
	(footprint "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
		(layer "F.Cu")
		(uuid "81e8f08a-599a-4871-8675-facc04664c87")
		(at 147.6375 42.8625)
		(property "Reference" "MX7"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
			(uuid "6421fbc4-485c-45e2-a60f-db3f26bb1310")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "MX_SW_HS"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "f76943f8-baaf-4288-8a90-91c64bfe36b5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "68217ede-1df3-4fa5-9199-20dbb735d9d2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "4850688a-e601-4fc9-a89c-308cc982e43b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted, Kailh CPG151101S11 for Cherry MX style switches"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "36233672-b84b-4177-9a0e-965e38d17ec8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/3e0103d0-3c8c-48bf-b97a-03698bcbf672")
		(sheetname "Stammblatt")
		(sheetfile "geebord-plate.kicad_sch")
		(attr exclude_from_pos_files allow_missing_courtyard)
		(fp_rect
			(start -9.525 -9.525)
			(end 9.525 9.525)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "Dwgs.User")
			(uuid "bbd89983-9a59-4ad6-bd26-cd08d3a545b9")
		)
		(fp_line
			(start -7 -6.5)
			(end -7 6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "36c5bc74-bbee-4eb4-b1b6-08f8b919d9d7")
		)
		(fp_line
			(start -6.5 7)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "9452fade-2da8-4977-800d-5dd95ff8eb08")
		)
		(fp_line
			(start 6.5 -7)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "f85229cc-b51f-43a6-9c32-c031aa01c19b")
		)
		(fp_line
			(start 7 6.5)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "8284dbd3-5b13-4a6d-b6af-d97295d8501d")
		)
		(fp_arc
			(start -7 -6.5)
			(mid -6.853553 -6.853553)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "73b7a329-d9da-4a92-bf7a-2f127cbc516c")
		)
		(fp_arc
			(start -6.497236 6.998884)
			(mid -6.850789 6.852437)
			(end -6.997236 6.498884)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "ee3b5f68-b9a1-420b-bffa-c29a381c733e")
		)
		(fp_arc
			(start 6.5 -7)
			(mid 6.853553 -6.853553)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "1e6c9436-3f00-4758-9735-4fa9a4531756")
		)
		(fp_arc
			(start 7 6.5)
			(mid 6.853553 6.853553)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "18363880-aefd-4f08-b74c-8984f1f524b3")
		)
	)
	(footprint "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
		(layer "F.Cu")
		(uuid "83e46df0-3a31-466c-9781-739a38d5fc4a")
		(at 166.6875 42.8625)
		(property "Reference" "MX8"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
			(uuid "aa860bd8-38d3-43db-85c3-4e8db97c8779")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "MX_SW_HS"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "c1221ed4-e442-4953-8496-3fdc52f42037")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "a3b419ca-3757-418f-affe-3a7488709518")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "87663b5e-0e95-4e46-b7fe-f50e1a45fa27")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted, Kailh CPG151101S11 for Cherry MX style switches"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "a36b04dd-6380-4416-86d3-7aa2cc3ffa23")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/bb2bf9d9-625f-4c3c-948c-f30dc8ea2857")
		(sheetname "Stammblatt")
		(sheetfile "geebord-plate.kicad_sch")
		(attr exclude_from_pos_files allow_missing_courtyard)
		(fp_rect
			(start -9.525 -9.525)
			(end 9.525 9.525)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "Dwgs.User")
			(uuid "b232f124-d49e-49e7-b00f-08577c37d189")
		)
		(fp_line
			(start -7 -6.5)
			(end -7 6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "81751a1d-2c88-48b7-8807-d10a2411d644")
		)
		(fp_line
			(start -6.5 7)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "95b4b365-8249-4d0c-a597-6b92d41bccf1")
		)
		(fp_line
			(start 6.5 -7)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "def7d05b-9d2c-465d-8c00-53c2c1943149")
		)
		(fp_line
			(start 7 6.5)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "c3be2a17-fb3e-4114-89c8-9d4d87b52065")
		)
		(fp_arc
			(start -7 -6.5)
			(mid -6.853553 -6.853553)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "0ca833e7-8bec-45ac-bca9-797fa555d624")
		)
		(fp_arc
			(start -6.497236 6.998884)
			(mid -6.850789 6.852437)
			(end -6.997236 6.498884)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "49cab92d-acdb-40cb-bfc8-44ca08c8bd61")
		)
		(fp_arc
			(start 6.5 -7)
			(mid 6.853553 -6.853553)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "8c702635-a8bf-4e50-ae6e-ca70c5090272")
		)
		(fp_arc
			(start 7 6.5)
			(mid 6.853553 6.853553)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "f7e17ab5-9ef4-4f37-a30b-6aa61e3f206d")
		)
	)
	(footprint "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
		(layer "F.Cu")
		(uuid "8677f64f-f9c3-4b1d-8072-6e3b6dd334ed")
		(at 90.4875 100.0125)
		(property "Reference" "MX40"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
			(uuid "43bf0693-d965-4add-b8bd-f972f5543099")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "MX_SW_HS"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "f1e2b6c8-312e-4a4f-b06f-faca1249c10c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "bb89028a-ec11-4200-9dbd-88a3d915979a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "ea4c7f94-e19e-427d-bca6-76249fc2fe8b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted, Kailh CPG151101S11 for Cherry MX style switches"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "38cb1abd-1ab1-44fb-b6c7-bfdf8a5439fc")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/bb498b8b-a19c-45fe-82a4-80b588b600d7")
		(sheetname "Stammblatt")
		(sheetfile "geebord-plate.kicad_sch")
		(attr exclude_from_pos_files allow_missing_courtyard)
		(fp_rect
			(start -9.525 -9.525)
			(end 9.525 9.525)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "Dwgs.User")
			(uuid "0f8ff6d7-403e-41d0-9031-ecd076ef04d7")
		)
		(fp_line
			(start -7 -6.5)
			(end -7 6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "9cd28b40-3d7f-4b40-b45d-30b0974108f9")
		)
		(fp_line
			(start -6.5 7)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "ce6b4553-b831-41c2-9ff7-4c5dc3ecefd1")
		)
		(fp_line
			(start 6.5 -7)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "4e33d13c-3fc2-4bbf-bded-dc1929c488bd")
		)
		(fp_line
			(start 7 6.5)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "9cdb180f-1ba3-424f-8e07-2402c196bd55")
		)
		(fp_arc
			(start -7 -6.5)
			(mid -6.853553 -6.853553)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "b3a9320e-8fa2-43df-ad2c-91ef160e2930")
		)
		(fp_arc
			(start -6.497236 6.998884)
			(mid -6.850789 6.852437)
			(end -6.997236 6.498884)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "a5ab7e1c-52d5-43e5-abc3-a46ac236759d")
		)
		(fp_arc
			(start 6.5 -7)
			(mid 6.853553 -6.853553)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "899973b7-b68f-4d6f-9d00-da5d75bf6322")
		)
		(fp_arc
			(start 7 6.5)
			(mid 6.853553 6.853553)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "f67070d1-9c02-4183-b1f4-f9c4fb4eae13")
		)
	)
	(footprint "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
		(layer "F.Cu")
		(uuid "8f2217f3-a67e-45ab-a1b1-508d998b90b5")
		(at 128.5875 42.8625)
		(property "Reference" "MX6"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
			(uuid "e7290b44-a25f-40ea-8ec2-40fe64c105b5")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "MX_SW_HS"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "e8840185-9904-45b6-9fe8-dafd89368e28")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "c4948267-1b7f-48ac-9779-8e9409716a7c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "6700a6f1-a6a2-48ca-a6f0-468056186403")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted, Kailh CPG151101S11 for Cherry MX style switches"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "ef4a32b0-915c-49cd-b16d-01a4e512f4a2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/47c77e78-2974-441a-9fa5-05af5d379e11")
		(sheetname "Stammblatt")
		(sheetfile "geebord-plate.kicad_sch")
		(attr exclude_from_pos_files allow_missing_courtyard)
		(fp_rect
			(start -9.525 -9.525)
			(end 9.525 9.525)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "Dwgs.User")
			(uuid "91bb0672-a9bb-4ae7-bcb1-4628082453f0")
		)
		(fp_line
			(start -7 -6.5)
			(end -7 6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "f68c961f-71b1-46e2-8af1-98418d86cffe")
		)
		(fp_line
			(start -6.5 7)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "ef88762a-001a-4309-bebc-4a4bfdb956fa")
		)
		(fp_line
			(start 6.5 -7)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "6c831788-bf79-4fdd-be3f-338aca258e23")
		)
		(fp_line
			(start 7 6.5)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "8c9a9bd1-914e-42e1-97d6-a44bdbba22a5")
		)
		(fp_arc
			(start -7 -6.5)
			(mid -6.853553 -6.853553)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "66686e09-630c-4ed1-84d2-f72c7c04f139")
		)
		(fp_arc
			(start -6.497236 6.998884)
			(mid -6.850789 6.852437)
			(end -6.997236 6.498884)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "5033c542-bb8d-457a-8442-398f7a2619f7")
		)
		(fp_arc
			(start 6.5 -7)
			(mid 6.853553 -6.853553)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "e443708b-54a6-43b4-aa2a-3ccbd02ea5f7")
		)
		(fp_arc
			(start 7 6.5)
			(mid 6.853553 6.853553)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "d4f10896-0b2b-4b23-a519-d6b043983f45")
		)
	)
	(footprint "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
		(layer "F.Cu")
		(uuid "9cada7ad-084e-4d08-90ca-d4ae159c8d5a")
		(at 52.3875 100.0125)
		(property "Reference" "MX38"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
			(uuid "370efc36-285e-4d3a-8e9d-deb13f211b32")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "MX_SW_HS"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "60d187ff-4ea6-4e2e-823d-058f21e6a0d6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "4ab6d05b-ae6d-47c4-8137-be3f01571eff")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "1c7c3d3c-36ae-4ef4-af3b-d52f512598ff")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted, Kailh CPG151101S11 for Cherry MX style switches"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "339f4dd9-30b1-42e7-9bee-446e24150c37")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/c7214820-a559-4e84-90f9-df170eaca21f")
		(sheetname "Stammblatt")
		(sheetfile "geebord-plate.kicad_sch")
		(attr exclude_from_pos_files allow_missing_courtyard)
		(fp_rect
			(start -9.525 -9.525)
			(end 9.525 9.525)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "Dwgs.User")
			(uuid "f5b77764-f5dc-40d5-8ba8-137249c433c7")
		)
		(fp_line
			(start -7 -6.5)
			(end -7 6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "206fe55c-2896-431f-baca-9c6b2f83c00d")
		)
		(fp_line
			(start -6.5 7)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "ba00b635-67c8-4d64-adf2-95c213151a09")
		)
		(fp_line
			(start 6.5 -7)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "a02a6cca-4f34-4535-8349-b3ecae58bd24")
		)
		(fp_line
			(start 7 6.5)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "60a03fea-5496-4b2d-ae99-8ca1839340bb")
		)
		(fp_arc
			(start -7 -6.5)
			(mid -6.853553 -6.853553)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "6d13216f-9297-4189-9a95-69fc12bb951d")
		)
		(fp_arc
			(start -6.497236 6.998884)
			(mid -6.850789 6.852437)
			(end -6.997236 6.498884)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "e534972d-03a4-4326-930a-75edc61dbfaf")
		)
		(fp_arc
			(start 6.5 -7)
			(mid 6.853553 -6.853553)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "c77f9bbf-a9cd-4de2-97b1-f9695c0c6da5")
		)
		(fp_arc
			(start 7 6.5)
			(mid 6.853553 6.853553)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "498aa3bc-e1f7-4b23-a899-4051415d2ce7")
		)
	)
	(footprint "geebord-library:JOYSTICK_ANALOG_MINITHM"
		(layer "F.Cu")
		(uuid "a7534fb8-5e47-47f4-8155-4db2361cf4b2")
		(at 138.0932 99.9828 90)
		(property "Reference" "JS1"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
			(uuid "2ad979ed-784c-4e87-bf34-85fd9ca3a2b5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "joystick_analog"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "811f7c2f-4845-429f-b3fe-4ae9b7538990")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "geebord-library:JOYSTICK_ANALOG_MINITHM"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "9c6fc3ad-5cb2-44dd-9725-71ca62af8947")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "377b8018-145f-4aae-a6dd-33d8c7f4062e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "37a65053-1a8c-4e13-8b24-02ea6aa7c894")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/0fadd9f7-beab-4f1c-846c-032f69da825f")
		(sheetname "Stammblatt")
		(sheetfile "geebord-plate.kicad_sch")
		(fp_line
			(start 6 -9)
			(end 9 -6)
			(stroke
				(width 0.127)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "1bdc7173-0d54-483b-a04e-c9b3140b8482")
		)
		(fp_line
			(start -6 -9)
			(end 6 -9)
			(stroke
				(width 0.127)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "9cd480b3-616a-409c-8950-4b08d3bd9001")
		)
		(fp_line
			(start 9 -6)
			(end 9 6)
			(stroke
				(width 0.127)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "c1c3de63-64f1-4af9-ab10-312784e647ec")
		)
		(fp_line
			(start -9 -6)
			(end -6 -9)
			(stroke
				(width 0.127)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "605b0026-5f08-4f2e-8392-1bcda24b9a2d")
		)
		(fp_line
			(start 9 6)
			(end 6 9)
			(stroke
				(width 0.127)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "11b7deb6-d510-4ff2-a662-8a93b395e0a7")
		)
		(fp_line
			(start -9 6)
			(end -9 -6)
			(stroke
				(width 0.127)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "015dec30-8d40-496b-8c38-ce7f0f7f9370")
		)
		(fp_line
			(start 6 9)
			(end -6 9)
			(stroke
				(width 0.127)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "4c5dd8ec-db52-46f8-bcab-6ec052f71595")
		)
		(fp_line
			(start -6 9)
			(end -9 6)
			(stroke
				(width 0.127)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "cf965342-d70b-4a55-8d06-bee41955ca7b")
		)
		(fp_circle
			(center 0 0)
			(end 7 0)
			(stroke
				(width 0.127)
				(type solid)
			)
			(fill none)
			(layer "F.SilkS")
			(uuid "78ba86a1-9f06-46c6-8c0a-ab44268df40e")
		)
		(fp_poly
			(pts
				(xy 0.467692 -5.64421) (xy 0.932191 -5.58631) (xy 1.390321 -5.490251) (xy 1.838953 -5.356688) (xy 2.275024 -5.186532)
				(xy 2.695554 -4.980947) (xy 3.097671 -4.741338) (xy 3.478627 -4.46934) (xy 3.835821 -4.166812) (xy 4.166812 -3.835821)
				(xy 4.46934 -3.478627) (xy 4.741338 -3.097671) (xy 4.980947 -2.695554) (xy 5.186532 -2.275024) (xy 5.356688 -1.838953)
				(xy 5.490251 -1.390321) (xy 5.586581 -0.930903) (xy 5.663609 -0.001315) (xy 5.64421 0.467692) (xy 5.58631 0.932191)
				(xy 5.490251 1.390321) (xy 5.356688 1.838953) (xy 5.186532 2.275024) (xy 4.980947 2.695554) (xy 4.741338 3.097671)
				(xy 4.46934 3.478627) (xy 4.166812 3.835821) (xy 3.835821 4.166812) (xy 3.478627 4.46934) (xy 3.097671 4.741338)
				(xy 2.695554 4.980947) (xy 2.275024 5.186532) (xy 1.838953 5.356688) (xy 1.390321 5.490251) (xy 0.932191 5.58631)
				(xy 0.467692 5.64421) (xy 0 5.663554) (xy -0.467692 5.64421) (xy -0.932191 5.58631) (xy -1.390321 5.490251)
				(xy -1.838953 5.356688) (xy -2.275024 5.186532) (xy -2.695554 4.980947) (xy -3.097671 4.741338)
				(xy -3.478627 4.46934) (xy -3.835821 4.166812) (xy -4.166812 3.835821) (xy -4.46934 3.478627) (xy -4.741338 3.097671)
				(xy -4.980947 2.695554) (xy -5.186532 2.275024) (xy -5.356688 1.838953) (xy -5.490251 1.390321)
				(xy -5.58631 0.932191) (xy -5.64421 0.467692) (xy -5.663554 0) (xy -5.64421 -0.467692) (xy -5.58631 -0.932191)
				(xy -5.490251 -1.390321) (xy -5.356688 -1.838953) (xy -5.186532 -2.275024) (xy -4.980947 -2.695554)
				(xy -4.741338 -3.097671) (xy -4.46934 -3.478627) (xy -4.166812 -3.835821) (xy -3.835821 -4.166812)
				(xy -3.478627 -4.46934) (xy -3.097671 -4.741338) (xy -2.695554 -4.980947) (xy -2.275024 -5.186532)
				(xy -1.838953 -5.356688) (xy -1.390321 -5.490251) (xy -0.932191 -5.58631) (xy -0.467692 -5.64421)
				(xy 0 -5.663554)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill solid)
			(layer "F.SilkS")
			(uuid "d0e740aa-9c96-4f77-bd10-b013c5878b5d")
		)
		(fp_text user "<-X"
			(at 11 -4 180)
			(unlocked yes)
			(layer "B.SilkS")
			(uuid "b8e4ffdc-af9f-454c-a803-5b818ea94aee")
			(effects
				(font
					(size 1.0922 1.0922)
					(thickness 0.1778)
				)
				(justify left bottom)
			)
		)
		(fp_text user "<-Y"
			(at 7.571 -7.81 90)
			(unlocked yes)
			(layer "B.SilkS")
			(uuid "fafa0f6e-899e-4496-bae5-45a58ef2c1c4")
			(effects
				(font
					(size 1.0922 1.0922)
					(thickness 0.1778)
				)
				(justify left bottom)
			)
		)
		(pad "" np_thru_hole circle
			(at -6 -6 90)
			(size 1.6 1.6)
			(drill 1.6)
			(layers "*.Cu" "*.Mask")
			(uuid "a7c068e8-9704-4eea-9008-43c3c0327fcc")
		)
		(pad "" np_thru_hole circle
			(at 6 6 90)
			(size 1.6 1.6)
			(drill 1.6)
			(layers "*.Cu" "*.Mask")
			(uuid "86b54fd7-4617-4003-b900-3a1c3b70e5a3")
		)
		(pad "1" thru_hole oval
			(at 0 -9 180)
			(size 3 1.5)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(J1-Pin_3)")
			(pinfunction "X")
			(pintype "output")
			(solder_mask_margin 0.0508)
			(thermal_bridge_angle 0)
			(uuid "7b0eb75b-e355-4c2e-8f7b-03cbdb973a14")
		)
		(pad "2" thru_hole oval
			(at -2 -9 180)
			(size 3 1.5)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "Net-(J1-Pin_4)")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.0508)
			(thermal_bridge_angle 0)
			(uuid "3647b5f0-a5e4-4669-8a70-1f21b811d0ca")
		)
		(pad "2" thru_hole oval
			(at 9 2 90)
			(size 3 1.5)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "Net-(J1-Pin_4)")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.0508)
			(thermal_bridge_angle 0)
			(uuid "a118b915-919d-4d51-9ee8-4134c379a84e")
		)
		(pad "3" thru_hole oval
			(at 9 0 90)
			(size 3 1.5)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "Net-(J1-Pin_2)")
			(pinfunction "Y")
			(pintype "output")
			(solder_mask_margin 0.0508)
			(thermal_bridge_angle 0)
			(uuid "752743f7-78ec-4402-a116-01ea20875314")
		)
		(pad "4" thru_hole oval
			(at 2 -9 180)
			(size 3 1.5)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(J1-Pin_1)")
			(pinfunction "VCC")
			(pintype "power_in")
			(solder_mask_margin 0.0508)
			(thermal_bridge_angle 0)
			(uuid "54be4d8a-88a3-4dff-b42c-878c35476db4")
		)
		(pad "4" thru_hole oval
			(at 9 -2 90)
			(size 3 1.5)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(J1-Pin_1)")
			(pinfunction "VCC")
			(pintype "power_in")
			(solder_mask_margin 0.0508)
			(thermal_bridge_angle 0)
			(uuid "d52ae603-9fdd-4553-9a08-1d19c4e62b58")
		)
	)
	(footprint "PCM_marbastlib-xp-plate-mx:Plate_MX_1.5u"
		(layer "F.Cu")
		(uuid "a9f0bd16-34aa-41d1-9449-a42ba48b7217")
		(at 114.3 100.0125)
		(property "Reference" "MX41"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
			(uuid "2728761c-8ffa-44ed-ab60-33675f483c16")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "MX_SW_HS"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "e56df75d-aec3-4fbc-9324-b384f74cf608")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "PCM_marbastlib-xp-plate-mx:Plate_MX_1.5u"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "e8dd9828-bd0e-4953-8670-a59496a47c8e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "d6273a14-03c1-49d4-bd92-ff6962899e69")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted, Kailh CPG151101S11 for Cherry MX style switches"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "d138f6a1-8a6c-4862-aaa0-9ee9df2e25cb")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/52f15005-3911-4322-9144-92f0f4c2706b")
		(sheetname "Stammblatt")
		(sheetfile "geebord-plate.kicad_sch")
		(attr exclude_from_pos_files allow_missing_courtyard)
		(fp_rect
			(start -14.2875 -9.525)
			(end 14.2875 9.525)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "Dwgs.User")
			(uuid "8ec3cad8-8200-49da-bf55-75b843ba6714")
		)
		(fp_line
			(start -7 -6.5)
			(end -7 6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "f0b84edd-a22e-44ce-975a-3ed132711d1b")
		)
		(fp_line
			(start -6.5 7)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "83632e94-108f-4cd4-867b-999bd76f2d38")
		)
		(fp_line
			(start 6.5 -7)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "a441f73e-f769-40f2-aec9-8e727889a4ff")
		)
		(fp_line
			(start 7 6.5)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "2852f977-8365-40a7-851c-3824c6b83a9d")
		)
		(fp_arc
			(start -7 -6.5)
			(mid -6.853553 -6.853553)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "8c8e0fbc-bcfe-4992-8e63-d90fcdddce4d")
		)
		(fp_arc
			(start -6.497236 6.998884)
			(mid -6.850789 6.852437)
			(end -6.997236 6.498884)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "96226c13-fcc1-495a-ba4b-b4d33ada0b71")
		)
		(fp_arc
			(start 6.5 -7)
			(mid 6.853553 -6.853553)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "1c916773-5b6c-41cd-94e1-7b7ede5cca70")
		)
		(fp_arc
			(start 7 6.5)
			(mid 6.853553 6.853553)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "5c6c5feb-4ac0-4c44-bf88-052bab3066d0")
		)
	)
	(footprint "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
		(layer "F.Cu")
		(uuid "afa3eba2-b515-4d3f-96af-29d6a8a06168")
		(at 204.7875 100.0125)
		(property "Reference" "MX44"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
			(uuid "febc618f-c665-4db9-a698-3a6bf969a7b8")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "MX_SW_HS"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "5d421d31-7c60-4fb0-9f1e-66b3ab6f5efa")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "1c97d774-f954-465b-b4cc-71757b21e0d5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "07443435-2e03-4887-9bb2-a2af370709b9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted, Kailh CPG151101S11 for Cherry MX style switches"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "18914be8-f56e-4338-bc07-447bb3e1a73f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/2823dfdc-c80a-42c9-b943-a6b04f4f175d")
		(sheetname "Stammblatt")
		(sheetfile "geebord-plate.kicad_sch")
		(attr exclude_from_pos_files allow_missing_courtyard)
		(fp_rect
			(start -9.525 -9.525)
			(end 9.525 9.525)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "Dwgs.User")
			(uuid "585b0631-1ff1-4eee-aa61-d882f8347e41")
		)
		(fp_line
			(start -7 -6.5)
			(end -7 6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "a4d94a8e-a8b1-48b6-848f-7ae554f68d81")
		)
		(fp_line
			(start -6.5 7)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "f808ced1-2b40-4a50-be50-0c02b76f0647")
		)
		(fp_line
			(start 6.5 -7)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "1894b0a8-2771-45a7-920e-769bf2e4d225")
		)
		(fp_line
			(start 7 6.5)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "496c5635-bee4-4e39-a4a8-48d9bd38ad9c")
		)
		(fp_arc
			(start -7 -6.5)
			(mid -6.853553 -6.853553)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "2cbea09a-afb8-4dee-b6e5-702665b6d155")
		)
		(fp_arc
			(start -6.497236 6.998884)
			(mid -6.850789 6.852437)
			(end -6.997236 6.498884)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "73efcf03-29f3-4ada-b83b-7406c6d22916")
		)
		(fp_arc
			(start 6.5 -7)
			(mid 6.853553 -6.853553)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "d1edba8d-a645-496d-83a3-3a52ca865b60")
		)
		(fp_arc
			(start 7 6.5)
			(mid 6.853553 6.853553)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "e66a25df-75c3-4e8a-8aa0-e493bf85c351")
		)
	)
	(footprint "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
		(layer "F.Cu")
		(uuid "b5ad84cf-7c50-4adf-ad0f-68f4cc515ba9")
		(at 204.7875 42.8625)
		(property "Reference" "MX10"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
			(uuid "158c1f5b-bb7e-4025-bf54-6dc3ad3c2fee")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "MX_SW_HS"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "c1ef6956-a448-494a-83e6-4ea4e5c8fb72")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "f16fe36c-0add-4a91-be7c-5cb8d8cd52d8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "a8d97142-8736-44b4-a9ee-886b08f04950")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted, Kailh CPG151101S11 for Cherry MX style switches"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "2c9d2703-ef91-4575-b297-23409813c4f6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/e66dde52-5887-4fb2-9049-aeac4c7cae7e")
		(sheetname "Stammblatt")
		(sheetfile "geebord-plate.kicad_sch")
		(attr exclude_from_pos_files allow_missing_courtyard)
		(fp_rect
			(start -9.525 -9.525)
			(end 9.525 9.525)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "Dwgs.User")
			(uuid "b8ae1dcb-e61a-40ee-977f-1bda00d8eaf5")
		)
		(fp_line
			(start -7 -6.5)
			(end -7 6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "1968b55e-26af-4363-b759-037e8a0300dc")
		)
		(fp_line
			(start -6.5 7)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "1150a12f-0dcb-4b68-8ff8-876fe1a13f48")
		)
		(fp_line
			(start 6.5 -7)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "fdd05255-6305-4588-8a56-f527a253162a")
		)
		(fp_line
			(start 7 6.5)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "2d79d759-8b23-4815-93b0-ef527fb2a52a")
		)
		(fp_arc
			(start -7 -6.5)
			(mid -6.853553 -6.853553)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "d1bbad05-9a37-44f8-86a8-5c4324adbddb")
		)
		(fp_arc
			(start -6.497236 6.998884)
			(mid -6.850789 6.852437)
			(end -6.997236 6.498884)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "b524bb2c-30bf-4640-af0c-18d58b04b7a8")
		)
		(fp_arc
			(start 6.5 -7)
			(mid 6.853553 -6.853553)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "94497e75-a662-4698-bf80-1e77ea5587a0")
		)
		(fp_arc
			(start 7 6.5)
			(mid 6.853553 6.853553)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "be801df8-bb85-4ac4-8f76-3e5a18a9bff3")
		)
	)
	(footprint "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
		(layer "F.Cu")
		(uuid "bd52c1ff-509a-4961-a0af-509e5f62c93b")
		(at 33.3375 42.8625)
		(property "Reference" "MX1"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
			(uuid "78be0d56-54eb-4f73-990a-54d245901f61")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "MX_SW_HS"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "42b6c586-8fde-4e37-a71c-84be259de46d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "a21a9121-7c1b-405b-860c-1983c32c9c1d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "8be82782-c637-4f9b-bc0d-87205a3f9e41")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted, Kailh CPG151101S11 for Cherry MX style switches"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "b6fbfdf4-39f1-48e7-9d62-f0418739ffde")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/330af517-c5ba-4357-97dc-d65d6d45623c")
		(sheetname "Stammblatt")
		(sheetfile "geebord-plate.kicad_sch")
		(attr exclude_from_pos_files allow_missing_courtyard)
		(fp_rect
			(start -9.525 -9.525)
			(end 9.525 9.525)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "Dwgs.User")
			(uuid "a119d858-2b33-4bc8-8254-7d9e977501c4")
		)
		(fp_line
			(start -7 -6.5)
			(end -7 6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "b50d9f14-bef1-4745-82c2-1b38aacee3e2")
		)
		(fp_line
			(start -6.5 7)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "7e210e80-9d74-49fd-80de-0fceeb8c15b1")
		)
		(fp_line
			(start 6.5 -7)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "ccb3017f-e4e0-41ba-adfd-55cc12c045b4")
		)
		(fp_line
			(start 7 6.5)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "56f1ab94-f0e1-4f65-af89-645d7e488a10")
		)
		(fp_arc
			(start -7 -6.5)
			(mid -6.853553 -6.853553)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "14e0f6f9-346e-4133-8715-0841c5a2aa24")
		)
		(fp_arc
			(start -6.497236 6.998884)
			(mid -6.850789 6.852437)
			(end -6.997236 6.498884)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "c06063ce-476a-4de1-a996-32c855e6a85d")
		)
		(fp_arc
			(start 6.5 -7)
			(mid 6.853553 -6.853553)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "00d16ccf-d09c-4400-a25a-fb52625b9844")
		)
		(fp_arc
			(start 7 6.5)
			(mid 6.853553 6.853553)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "2bb8d7cc-79cb-4900-8fe4-b7e88af47486")
		)
		(model "${KICAD8_3RD_PARTY}/3dmodels/com_github_perigoso_keyswitch-kicad-library/3d-library.3dshapes/SW_Cherry_MX_Plate.stp"
			(offset
				(xyz 0 0 -5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
		(layer "F.Cu")
		(uuid "c06d2257-4249-46ef-8e84-f5e8aad9f83d")
		(at 52.3875 61.9125)
		(property "Reference" "MX14"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
			(uuid "47dc9ae3-a7d6-4f96-b029-bc11c4cec649")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "MX_SW_HS"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "eb308ab4-aa9f-4bff-9d98-d9995773157f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "aed8012f-ea61-4df9-89fb-cd7d6cef5585")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "1b8ee5d4-edf8-4ec1-b020-a37f4a77498a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted, Kailh CPG151101S11 for Cherry MX style switches"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "50add4af-6264-4a52-84cf-24b5a3f4e887")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/4e9ed225-7263-4a96-8d73-64c62f6e8ff3")
		(sheetname "Stammblatt")
		(sheetfile "geebord-plate.kicad_sch")
		(attr exclude_from_pos_files allow_missing_courtyard)
		(fp_rect
			(start -9.525 -9.525)
			(end 9.525 9.525)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "Dwgs.User")
			(uuid "22579882-e1b3-4a18-8b31-58935c9b4cc4")
		)
		(fp_line
			(start -7 -6.5)
			(end -7 6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "ee0fba40-5186-4794-b1ed-5c0a857345e7")
		)
		(fp_line
			(start -6.5 7)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "6ef1590b-7fc0-4fe5-9ce5-15a3590f9f6c")
		)
		(fp_line
			(start 6.5 -7)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "9118ecc0-882e-49cb-95cc-d8a2894baf06")
		)
		(fp_line
			(start 7 6.5)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "3675e8b3-2796-4c6b-9293-b00c19c2bfbe")
		)
		(fp_arc
			(start -7 -6.5)
			(mid -6.853553 -6.853553)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "70b94106-15a5-4fdd-a0c4-ccc7320a8856")
		)
		(fp_arc
			(start -6.497236 6.998884)
			(mid -6.850789 6.852437)
			(end -6.997236 6.498884)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "5bde8f7c-4f85-411d-8896-241c4b8c686f")
		)
		(fp_arc
			(start 6.5 -7)
			(mid 6.853553 -6.853553)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "14a8c893-b864-4e54-a007-280b644214d1")
		)
		(fp_arc
			(start 7 6.5)
			(mid 6.853553 6.853553)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "ad2a6e9a-1a49-4e9d-97bb-53e6e5a72083")
		)
	)
	(footprint "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
		(layer "F.Cu")
		(uuid "c15ca476-b90a-48cf-acbd-e7fd1dd75982")
		(at 223.8375 100.0125)
		(property "Reference" "MX45"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
			(uuid "f7f1bd70-4d98-4f78-aee8-fdb291af317f")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "MX_SW_HS"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "d118d236-bbc1-49f7-814f-7328e0fe67b7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "9a568ca8-e0fe-4155-bd12-ca2a8185f690")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "9f961ea0-70f6-4182-82dc-13285e62727c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted, Kailh CPG151101S11 for Cherry MX style switches"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "452d35f5-3cb7-48e6-af97-43cd5ef71ea1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/7c95a97c-3607-44d6-b284-6a02a9b49b14")
		(sheetname "Stammblatt")
		(sheetfile "geebord-plate.kicad_sch")
		(attr exclude_from_pos_files allow_missing_courtyard)
		(fp_rect
			(start -9.525 -9.525)
			(end 9.525 9.525)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "Dwgs.User")
			(uuid "62a350c2-5687-45b8-b809-11f74ce7b490")
		)
		(fp_line
			(start -7 -6.5)
			(end -7 6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "694652bb-739c-49a0-aabc-c22bc8bd6179")
		)
		(fp_line
			(start -6.5 7)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "a57427cd-5361-42bf-8490-3f7008d7d73f")
		)
		(fp_line
			(start 6.5 -7)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "fcc90d89-cf1c-4b09-8d43-92d1a1165a01")
		)
		(fp_line
			(start 7 6.5)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "3fb4c034-d04a-465f-bff4-a83a5f69de85")
		)
		(fp_arc
			(start -7 -6.5)
			(mid -6.853553 -6.853553)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "3223bd41-bc1c-4d1d-a2b1-93a396c16e29")
		)
		(fp_arc
			(start -6.497236 6.998884)
			(mid -6.850789 6.852437)
			(end -6.997236 6.498884)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "a7622897-3cde-49a8-a373-138ed3ddae5f")
		)
		(fp_arc
			(start 6.5 -7)
			(mid 6.853553 -6.853553)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "a6c2ca74-a8ab-43be-b708-46e00cb22845")
		)
		(fp_arc
			(start 7 6.5)
			(mid 6.853553 6.853553)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "5174784c-9381-4e8d-8290-3e6a027f5266")
		)
	)
	(footprint "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
		(layer "F.Cu")
		(uuid "cb7f8c65-768c-4f5f-b25c-83cd39bc5738")
		(at 242.8875 61.9125)
		(property "Reference" "MX24"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
			(uuid "f24d8269-2c84-4521-aa4f-0a465a81b8fe")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "MX_SW_HS"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "66e1365c-4809-4e39-afcc-db23b10d86a3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "3f85dfa7-77ae-4b16-9fe7-5f803aebcd26")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "910ad1fb-99af-43d4-a773-ceb34b284cdf")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted, Kailh CPG151101S11 for Cherry MX style switches"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "512a316d-d73f-471a-8afc-1006494c0a1d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/368deebe-827a-4b35-a351-ce8c771d14ee")
		(sheetname "Stammblatt")
		(sheetfile "geebord-plate.kicad_sch")
		(attr exclude_from_pos_files allow_missing_courtyard)
		(fp_rect
			(start -9.525 -9.525)
			(end 9.525 9.525)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "Dwgs.User")
			(uuid "2e58866e-8a69-4461-b045-6c242ce2ddcf")
		)
		(fp_line
			(start -7 -6.5)
			(end -7 6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "6b1b6d93-d690-444a-936e-8e1ddfced4d5")
		)
		(fp_line
			(start -6.5 7)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "adc3e58e-e5f4-494a-a783-85d6a162380a")
		)
		(fp_line
			(start 6.5 -7)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "039223d8-dc39-4175-af0b-dc1a98c1fcd5")
		)
		(fp_line
			(start 7 6.5)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "a8c0ea22-9a1f-402c-ae0e-187b371cef3a")
		)
		(fp_arc
			(start -7 -6.5)
			(mid -6.853553 -6.853553)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "f6cf010d-4d1a-4772-8947-a146f0445e79")
		)
		(fp_arc
			(start -6.497236 6.998884)
			(mid -6.850789 6.852437)
			(end -6.997236 6.498884)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "ef6f8307-397f-4722-bf84-ed240bf0e97a")
		)
		(fp_arc
			(start 6.5 -7)
			(mid 6.853553 -6.853553)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "18fc9bb3-5775-46ec-b88e-1969b8374594")
		)
		(fp_arc
			(start 7 6.5)
			(mid 6.853553 6.853553)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "b3587e9f-3b95-4ad6-9c45-7f36d83161ea")
		)
	)
	(footprint "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
		(layer "F.Cu")
		(uuid "ccd3c3a6-ce1c-40b4-802b-3c6aef3111ed")
		(at 33.3375 61.9125)
		(property "Reference" "MX13"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
			(uuid "8a7b0803-e82c-4fe2-8b1d-3b9beec85e83")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "MX_SW_HS"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "3765b32d-7227-454e-b99c-d0d4cec7ea0f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "800f05f3-55b9-46d7-9792-c48137f551be")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "edc7610b-8a6d-493c-ad7d-488d7c69a545")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted, Kailh CPG151101S11 for Cherry MX style switches"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "16030f4d-f063-4c65-af4b-2fc846f592a8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/028790f2-e502-41ea-80a7-45e169fd2f67")
		(sheetname "Stammblatt")
		(sheetfile "geebord-plate.kicad_sch")
		(attr exclude_from_pos_files allow_missing_courtyard)
		(fp_rect
			(start -9.525 -9.525)
			(end 9.525 9.525)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "Dwgs.User")
			(uuid "edf78718-8d44-41f8-b5c9-3a1d0bd8a5ce")
		)
		(fp_line
			(start -7 -6.5)
			(end -7 6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "4cb84148-1c97-46c3-9213-eadab3b626e8")
		)
		(fp_line
			(start -6.5 7)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "43c83b76-dae9-4b91-8e80-ca66b4dcd357")
		)
		(fp_line
			(start 6.5 -7)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "b8f2efa4-cb7b-4734-9238-9e10c0cb1e76")
		)
		(fp_line
			(start 7 6.5)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "d895d301-1896-4f54-8cbc-091e9a8b3db7")
		)
		(fp_arc
			(start -7 -6.5)
			(mid -6.853553 -6.853553)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "3922e53b-6ff2-4a24-ab0d-cd210e7daa64")
		)
		(fp_arc
			(start -6.497236 6.998884)
			(mid -6.850789 6.852437)
			(end -6.997236 6.498884)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "22428b8b-f70b-4e7a-8877-421c017b5d3c")
		)
		(fp_arc
			(start 6.5 -7)
			(mid 6.853553 -6.853553)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "2d697e94-e63a-440d-a407-78f2d6cae0c8")
		)
		(fp_arc
			(start 7 6.5)
			(mid 6.853553 6.853553)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "44ed353d-ef6b-4154-9111-d283952b4f50")
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad"
		(layer "F.Cu")
		(uuid "cf4f5d82-6b8e-42cc-8d30-3fdde86eed05")
		(at 256.1125 113.4375)
		(descr "Mounting Hole 3.2mm, M3, DIN965")
		(tags "mounting hole 3.2mm m3 din965")
		(property "Reference" "REF**"
			(at 0 -3.8 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "c090f790-3aa4-456f-9490-9d89ce5f09bb")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "MountingHole_3.2mm_M3_DIN965_Pad"
			(at 0 3.8 0)
			(layer "F.Fab")
			(uuid "6283cebb-7532-435f-b4c2-4f017731a592")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a29ed821-0419-4806-921a-978c25dd14e4")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "7df64655-b538-4c08-a366-564f9953c0c1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "f99240a4-bbb5-4e5d-9f78-2ac005d8c520")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_circle
			(center 0 0)
			(end 2.8 0)
			(stroke
				(width 0.15)
				(type solid)
			)
			(fill none)
			(layer "Cmts.User")
			(uuid "14b0cdd6-bbba-42f2-a31f-79ee6ccaaa74")
		)
		(fp_circle
			(center 0 0)
			(end 3.05 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill none)
			(layer "F.CrtYd")
			(uuid "827dbd4b-dab1-4b86-97dd-6a396a3b0395")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "a72e0a04-7b38-4b0f-ac6c-b64cd1d3a97a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 5.6 5.6)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(uuid "d2faf83e-a4e1-4aed-9968-28d60bd3cd52")
		)
	)
	(footprint "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
		(layer "F.Cu")
		(uuid "d5fe43d9-2bae-4f8d-8e33-915c33a5f69a")
		(at 185.7375 61.9125)
		(property "Reference" "MX21"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
			(uuid "ffdc0c8e-04d5-4b79-8d28-1ea17ce72e23")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "MX_SW_HS"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "3f25f6b8-1318-4a0a-8d8c-c812d9eb8454")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "11381907-08a0-4e63-98cc-ab25ed8b8ead")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "3b7a34dc-0507-4338-b411-a28c24d5f4d5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted, Kailh CPG151101S11 for Cherry MX style switches"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "f3192adf-bad6-4943-9e3e-c9c63fb7bb5a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/53c75d68-3fb0-443a-afd1-8ab0e167915a")
		(sheetname "Stammblatt")
		(sheetfile "geebord-plate.kicad_sch")
		(attr exclude_from_pos_files allow_missing_courtyard)
		(fp_rect
			(start -9.525 -9.525)
			(end 9.525 9.525)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "Dwgs.User")
			(uuid "5dbaf7cb-7c50-439e-aa5f-4e4c36d0e588")
		)
		(fp_line
			(start -7 -6.5)
			(end -7 6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "3e8a644b-ba14-4da2-82ba-4e4fdab58441")
		)
		(fp_line
			(start -6.5 7)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "4bfa09aa-294d-4fd5-8dd4-c838238f287f")
		)
		(fp_line
			(start 6.5 -7)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "d21bea5c-96a4-4d08-94e1-b5b0c0502d36")
		)
		(fp_line
			(start 7 6.5)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "afdf41ba-07b6-4e52-97a9-01b67969d847")
		)
		(fp_arc
			(start -7 -6.5)
			(mid -6.853553 -6.853553)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "e52565b6-57bc-4f10-b01c-4a73eeed7a99")
		)
		(fp_arc
			(start -6.497236 6.998884)
			(mid -6.850789 6.852437)
			(end -6.997236 6.498884)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "bc821f6d-e484-4440-bd80-323e314be817")
		)
		(fp_arc
			(start 6.5 -7)
			(mid 6.853553 -6.853553)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "dd24bfc0-d7c7-4a82-9b51-a7af5791b320")
		)
		(fp_arc
			(start 7 6.5)
			(mid 6.853553 6.853553)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "0f15fc07-73b9-4244-ae3b-48db420e8936")
		)
	)
	(footprint "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
		(layer "F.Cu")
		(uuid "d688cf98-7716-479e-a4c6-3785ecfb3518")
		(at 71.4375 61.9125)
		(property "Reference" "MX15"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
			(uuid "c85e196b-6499-44aa-b1d7-3978bb4b9b8d")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "MX_SW_HS"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "61b14def-f01b-48a8-8fb7-b8cd8bd6bb58")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "a0a7ca8f-ab4e-4335-a956-8a538f7bf1d3")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "cff60a95-0ec0-4874-9a7f-cb9e66265cd6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted, Kailh CPG151101S11 for Cherry MX style switches"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "0e6d9a47-714e-4496-96da-cfbeca486751")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/eadda4c6-f4f0-41b6-8240-f3ab912c6c3d")
		(sheetname "Stammblatt")
		(sheetfile "geebord-plate.kicad_sch")
		(attr exclude_from_pos_files allow_missing_courtyard)
		(fp_rect
			(start -9.525 -9.525)
			(end 9.525 9.525)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "Dwgs.User")
			(uuid "eab6396e-3023-4901-96dd-38a5a8129aea")
		)
		(fp_line
			(start -7 -6.5)
			(end -7 6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "b15f79b1-eb47-42ad-86d3-b3c9e6639099")
		)
		(fp_line
			(start -6.5 7)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "8d583c4a-2582-4caf-a84c-745de768c7d8")
		)
		(fp_line
			(start 6.5 -7)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "5c0e00dd-8713-4bca-847f-a317b482f3c5")
		)
		(fp_line
			(start 7 6.5)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "96d96cb5-32c6-4b11-b93d-b1aa03303fb1")
		)
		(fp_arc
			(start -7 -6.5)
			(mid -6.853553 -6.853553)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "5eac63cf-5657-4073-9ff3-99d723ce5a0e")
		)
		(fp_arc
			(start -6.497236 6.998884)
			(mid -6.850789 6.852437)
			(end -6.997236 6.498884)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "588117ab-4aef-44f5-bce2-729661ee4b10")
		)
		(fp_arc
			(start 6.5 -7)
			(mid 6.853553 -6.853553)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "5d3e29af-9289-4b08-9f4e-494b52ac6b38")
		)
		(fp_arc
			(start 7 6.5)
			(mid 6.853553 6.853553)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "16bae8f6-a938-4db5-bc1d-586a95f7d56e")
		)
	)
	(footprint "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
		(layer "F.Cu")
		(uuid "dba7b0c9-de6a-4d1d-b87e-42831f5d6364")
		(at 33.3375 80.9625)
		(property "Reference" "MX25"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
			(uuid "f7cc1090-ac5b-4648-b93a-6503035b4234")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "MX_SW_HS"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "329b0e87-b2ac-4d7d-8881-347385fe13eb")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "0d9e6118-c8ea-4fcf-beea-e71559c6b6fb")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "d3898273-4996-404d-88b0-69d37d000755")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted, Kailh CPG151101S11 for Cherry MX style switches"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "2fbd8735-f724-40fd-8dc2-8996bcb78774")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/76f44b09-3998-49e0-ab9b-c79e849dbe8a")
		(sheetname "Stammblatt")
		(sheetfile "geebord-plate.kicad_sch")
		(attr exclude_from_pos_files allow_missing_courtyard)
		(fp_rect
			(start -9.525 -9.525)
			(end 9.525 9.525)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "Dwgs.User")
			(uuid "a1173317-4e7a-4dac-98d1-300bba5101f9")
		)
		(fp_line
			(start -7 -6.5)
			(end -7 6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "ae142eb7-a610-4f1d-b629-33063cf7a19b")
		)
		(fp_line
			(start -6.5 7)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "35a684f9-4f02-4f9e-8775-9137b2f98ab5")
		)
		(fp_line
			(start 6.5 -7)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "922ef540-a2db-4ccf-8c20-9023c7b55b5a")
		)
		(fp_line
			(start 7 6.5)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "095fe717-f7c1-4181-9f09-92fb1cf8d2ae")
		)
		(fp_arc
			(start -7 -6.5)
			(mid -6.853553 -6.853553)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "495838a4-f944-4cb6-8b27-22446d6638ac")
		)
		(fp_arc
			(start -6.497236 6.998884)
			(mid -6.850789 6.852437)
			(end -6.997236 6.498884)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "f6b1a6c9-1c65-40fe-bfa1-9a4efc636c76")
		)
		(fp_arc
			(start 6.5 -7)
			(mid 6.853553 -6.853553)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "a9ee29df-12ba-490f-acc1-9236a8bdebb1")
		)
		(fp_arc
			(start 7 6.5)
			(mid 6.853553 6.853553)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "df686829-de56-4dce-83d8-5a20e99620ca")
		)
	)
	(footprint "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
		(layer "F.Cu")
		(uuid "dd92fb70-2284-4e48-8c97-d5dbc5f9833d")
		(at 223.8375 61.9125)
		(property "Reference" "MX23"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
			(uuid "1d840f50-4435-4c06-b508-d71cec46d8ac")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "MX_SW_HS"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "9080a29c-87d8-46d0-a000-6317beac97cb")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "21ba5561-3b5f-48dc-a5a0-c8b3b9b496d6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "274cde61-12c9-463a-884e-16456a175963")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted, Kailh CPG151101S11 for Cherry MX style switches"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "143a8c43-85b6-4ccb-945d-98584ab5033d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/ec3c9104-04e9-4d16-a493-74be2b2fb1a6")
		(sheetname "Stammblatt")
		(sheetfile "geebord-plate.kicad_sch")
		(attr exclude_from_pos_files allow_missing_courtyard)
		(fp_rect
			(start -9.525 -9.525)
			(end 9.525 9.525)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "Dwgs.User")
			(uuid "d463a05e-a57b-4495-8bc7-4e7a034a6070")
		)
		(fp_line
			(start -7 -6.5)
			(end -7 6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "008eed5b-eb89-4ccd-99e4-c8904b8fa409")
		)
		(fp_line
			(start -6.5 7)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "d7849336-c7be-406f-9a53-6690f1b8db67")
		)
		(fp_line
			(start 6.5 -7)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "0c02aeb5-94e9-4b78-89fb-978a87a7528d")
		)
		(fp_line
			(start 7 6.5)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "f3431c14-5ea4-4984-9da3-f574d54176bf")
		)
		(fp_arc
			(start -7 -6.5)
			(mid -6.853553 -6.853553)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "3696ca90-0e7f-4edb-b07d-15525012cde6")
		)
		(fp_arc
			(start -6.497236 6.998884)
			(mid -6.850789 6.852437)
			(end -6.997236 6.498884)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "daea200c-891d-4f67-ac9a-6766f9b0d20c")
		)
		(fp_arc
			(start 6.5 -7)
			(mid 6.853553 -6.853553)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "321111d1-1ee1-46d7-ad37-fe48d53ab5ef")
		)
		(fp_arc
			(start 7 6.5)
			(mid 6.853553 6.853553)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "0e7a1b2b-fd16-4963-8e57-49deda8af64d")
		)
	)
	(footprint "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
		(layer "F.Cu")
		(uuid "e1472cca-4177-4b6b-b704-481ad646645e")
		(at 147.6375 80.9625)
		(property "Reference" "MX31"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
			(uuid "52440400-4227-41bb-aa64-ce39def3e57f")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "MX_SW_HS"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "e978accc-3f51-46aa-ba0d-ac49b6e6f232")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "d0da9340-c38d-4389-964a-00a9590877bf")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "41d56707-7a76-4cee-9507-621b624e1945")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted, Kailh CPG151101S11 for Cherry MX style switches"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "0e57dfed-cdcf-4154-9b62-950ffeee8bd2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/d3e4ce17-3bf8-4ea7-9200-3074be03dd18")
		(sheetname "Stammblatt")
		(sheetfile "geebord-plate.kicad_sch")
		(attr exclude_from_pos_files allow_missing_courtyard)
		(fp_rect
			(start -9.525 -9.525)
			(end 9.525 9.525)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "Dwgs.User")
			(uuid "44092bc2-2272-4bdb-8cbf-dd4d009ff745")
		)
		(fp_line
			(start -7 -6.5)
			(end -7 6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "f7b19f9a-74e3-4352-b495-6c7b823c716a")
		)
		(fp_line
			(start -6.5 7)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "ebec53de-a067-47ec-9c83-1e6d4ba00b80")
		)
		(fp_line
			(start 6.5 -7)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "7cce0025-c7bc-4d33-87c7-8da8ada4b3a7")
		)
		(fp_line
			(start 7 6.5)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "eb1b4fbb-cf81-4c28-9ac6-e6f14917ac57")
		)
		(fp_arc
			(start -7 -6.5)
			(mid -6.853553 -6.853553)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "e79a7669-6e9a-4126-81d3-6185ef4fd087")
		)
		(fp_arc
			(start -6.497236 6.998884)
			(mid -6.850789 6.852437)
			(end -6.997236 6.498884)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "2d048348-ba4b-43be-a4e7-3a3d65284968")
		)
		(fp_arc
			(start 6.5 -7)
			(mid 6.853553 -6.853553)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "0ec39310-4c34-45d3-bacc-8be51ea12fcf")
		)
		(fp_arc
			(start 7 6.5)
			(mid 6.853553 6.853553)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "35c319c2-18be-47ea-b9f4-bc3c686c34ba")
		)
	)
	(footprint "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
		(layer "F.Cu")
		(uuid "e52e0f7e-2101-44e0-9b34-aa50d2943f7c")
		(at 33.3375 100.0125)
		(property "Reference" "MX37"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
			(uuid "beb957e9-454b-4751-8d5b-d4478caf13b9")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "MX_SW_HS"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "479b3140-4d69-4ed7-9d99-2ef3422ddbd8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "81c48397-3c1a-4bd2-93c7-7d7f660273a2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "16eca4f8-f467-48db-8e50-7b008419d412")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted, Kailh CPG151101S11 for Cherry MX style switches"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "1bf85f6a-502e-4dee-a659-494154857ad5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/ad28e3b0-963d-45f3-a511-f4616b320ae5")
		(sheetname "Stammblatt")
		(sheetfile "geebord-plate.kicad_sch")
		(attr exclude_from_pos_files allow_missing_courtyard)
		(fp_rect
			(start -9.525 -9.525)
			(end 9.525 9.525)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "Dwgs.User")
			(uuid "f28d607e-ea2c-4b7c-9953-039c4732827d")
		)
		(fp_line
			(start -7 -6.5)
			(end -7 6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "941f61e2-224f-49b6-bda8-446096b701e3")
		)
		(fp_line
			(start -6.5 7)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "5a9d9258-c4cd-486f-97d6-9c7cd55e562a")
		)
		(fp_line
			(start 6.5 -7)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "4180da83-f02c-4545-9b23-5f55100a6081")
		)
		(fp_line
			(start 7 6.5)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "e7fb15aa-7048-4075-9505-d44fb82747c4")
		)
		(fp_arc
			(start -7 -6.5)
			(mid -6.853553 -6.853553)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "76fe25f1-c667-4cd9-9249-afc39abbd558")
		)
		(fp_arc
			(start -6.497236 6.998884)
			(mid -6.850789 6.852437)
			(end -6.997236 6.498884)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "11be2b0e-bac5-4834-89ec-8d1e9239fd57")
		)
		(fp_arc
			(start 6.5 -7)
			(mid 6.853553 -6.853553)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "e52a99d4-effc-4ef2-9b91-9fdcabb944f8")
		)
		(fp_arc
			(start 7 6.5)
			(mid 6.853553 6.853553)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "85fa08a4-bdf8-4048-8b2c-a727dda00722")
		)
		(model "${KICAD8_3RD_PARTY}/3dmodels/com_github_perigoso_keyswitch-kicad-library/3d-library.3dshapes/SW_Cherry_MX_Plate.stp"
			(offset
				(xyz 0 0 -5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
		(layer "F.Cu")
		(uuid "e7cbd588-05e6-460e-ada5-ff91d0ff5c6f")
		(at 109.5375 80.9625)
		(property "Reference" "MX29"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
			(uuid "6407d888-90c5-4800-a523-960dd4228394")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "MX_SW_HS"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "f58567b7-5bb0-4fae-b11a-6dc3d02113f2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "79d3be0b-d022-4d81-bb44-0ae46bb7c192")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "69d1f3f9-0c04-47ad-8231-d0cdb7886eee")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted, Kailh CPG151101S11 for Cherry MX style switches"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "ff658c70-39aa-4ea3-8779-749921e4e2bc")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/6e934522-3834-44a5-9af2-dac1a9cb9820")
		(sheetname "Stammblatt")
		(sheetfile "geebord-plate.kicad_sch")
		(attr exclude_from_pos_files allow_missing_courtyard)
		(fp_rect
			(start -9.525 -9.525)
			(end 9.525 9.525)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "Dwgs.User")
			(uuid "61c7b057-f2d1-425c-9049-9deebf6e9ff7")
		)
		(fp_line
			(start -7 -6.5)
			(end -7 6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "880caca8-df2c-4281-b336-91f8dec0350d")
		)
		(fp_line
			(start -6.5 7)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "4ad84bc3-0525-41b5-840e-0854d279f9c4")
		)
		(fp_line
			(start 6.5 -7)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "690e642e-9c42-41a8-8fec-2a390262ddfd")
		)
		(fp_line
			(start 7 6.5)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "c9794410-a03e-4c33-8cdb-4faf5b002ba6")
		)
		(fp_arc
			(start -7 -6.5)
			(mid -6.853553 -6.853553)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "a704a02d-2e1b-45f7-a6b9-710d71d68598")
		)
		(fp_arc
			(start -6.497236 6.998884)
			(mid -6.850789 6.852437)
			(end -6.997236 6.498884)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "e400a59d-fef8-44f6-8bf4-b59e57f37d2a")
		)
		(fp_arc
			(start 6.5 -7)
			(mid 6.853553 -6.853553)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "18ee2644-9edb-4c68-944f-d62dbafdb173")
		)
		(fp_arc
			(start 7 6.5)
			(mid 6.853553 6.853553)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "be81a5fc-4346-4d82-9a73-1c4fe19bc4fb")
		)
	)
	(footprint "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
		(layer "F.Cu")
		(uuid "e99b6b18-ddc0-4e67-a580-d192e88f48d5")
		(at 52.3875 42.8625)
		(property "Reference" "MX2"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
			(uuid "ca4e96dc-56e0-4e9b-9afc-12ae088ab1e5")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "MX_SW_HS"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "3cb7736c-ab8d-4140-aaac-86c1e6bf6ff6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "d98bb8c6-71da-48a9-9dd4-ca2752e1b869")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "e74ca24d-5e1f-46d3-b558-c5509994c681")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted, Kailh CPG151101S11 for Cherry MX style switches"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "52bfcfda-d712-462d-9ade-e13745db09e2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/4d62c7e1-60a3-443f-81c5-a328dc27fdaa")
		(sheetname "Stammblatt")
		(sheetfile "geebord-plate.kicad_sch")
		(attr exclude_from_pos_files allow_missing_courtyard)
		(fp_rect
			(start -9.525 -9.525)
			(end 9.525 9.525)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "Dwgs.User")
			(uuid "318cf7cc-6332-4fd2-9773-d5cda1b5b56d")
		)
		(fp_line
			(start -7 -6.5)
			(end -7 6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "9b4f89b3-758d-45ac-852d-c723499287f3")
		)
		(fp_line
			(start -6.5 7)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "1aaf1354-b276-483e-a600-86c20b143813")
		)
		(fp_line
			(start 6.5 -7)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "0f85fee5-785b-4cce-8677-7b9e913164df")
		)
		(fp_line
			(start 7 6.5)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "97388c6f-2664-493a-8ca5-823ac719aca8")
		)
		(fp_arc
			(start -7 -6.5)
			(mid -6.853553 -6.853553)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "c3522dee-2140-4f49-a04d-a4d433b9a2aa")
		)
		(fp_arc
			(start -6.497236 6.998884)
			(mid -6.850789 6.852437)
			(end -6.997236 6.498884)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "adb34c69-54fd-4e28-8b14-bdff36092629")
		)
		(fp_arc
			(start 6.5 -7)
			(mid 6.853553 -6.853553)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "1291a82d-a5ff-41a0-8080-fb2c6f9ef83b")
		)
		(fp_arc
			(start 7 6.5)
			(mid 6.853553 6.853553)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "b2c9bb96-b73f-4005-81e3-364cf6d302e2")
		)
	)
	(footprint "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
		(layer "F.Cu")
		(uuid "eb87a81a-cde8-4a75-ba5d-57bce7b2a2c0")
		(at 90.4875 80.9625)
		(property "Reference" "MX28"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
			(uuid "659071ad-c0a0-43b1-b920-3815d9fd0dac")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "MX_SW_HS"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "35b35e28-1b96-46b5-9a75-ee86e04c43e3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "75be0f25-b31d-46a2-aefa-a23a331e4bf3")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "bfca0aa2-1201-4b11-ad12-1bed61e630be")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted, Kailh CPG151101S11 for Cherry MX style switches"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "41a264df-c7bc-445a-bc24-2739e28db9d4")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/0f20ff66-5f68-4bf5-991e-a752190afde9")
		(sheetname "Stammblatt")
		(sheetfile "geebord-plate.kicad_sch")
		(attr exclude_from_pos_files allow_missing_courtyard)
		(fp_rect
			(start -9.525 -9.525)
			(end 9.525 9.525)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "Dwgs.User")
			(uuid "72306672-5fc3-49f5-87bf-b58bc7252cfc")
		)
		(fp_line
			(start -7 -6.5)
			(end -7 6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "5aa147fb-02a9-47d1-8daa-bf6c6137a457")
		)
		(fp_line
			(start -6.5 7)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "01b13b72-5b20-4019-aea4-29ba29664ef8")
		)
		(fp_line
			(start 6.5 -7)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "4cee6a7f-d1c0-4817-aedf-8dbe7583c362")
		)
		(fp_line
			(start 7 6.5)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "e9982bca-9139-4af6-a860-6e06c2c23261")
		)
		(fp_arc
			(start -7 -6.5)
			(mid -6.853553 -6.853553)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "89eb1ad5-cf95-4662-97ad-94374c62fce9")
		)
		(fp_arc
			(start -6.497236 6.998884)
			(mid -6.850789 6.852437)
			(end -6.997236 6.498884)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "7359de6b-f295-4bce-a5de-2a445b5a297b")
		)
		(fp_arc
			(start 6.5 -7)
			(mid 6.853553 -6.853553)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "6e6b737a-6521-484b-a62f-ebd276ad667c")
		)
		(fp_arc
			(start 7 6.5)
			(mid 6.853553 6.853553)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "68117ce2-9ebe-4c39-8b36-ea7bad3f8fc2")
		)
	)
	(footprint "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
		(layer "F.Cu")
		(uuid "f262dbe0-2ff5-47cc-8851-8daafad50874")
		(at 52.3875 80.9625)
		(property "Reference" "MX26"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
			(uuid "8e858a1b-2667-4583-b1e7-3ee9792dcce5")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "MX_SW_HS"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "03917985-0802-429a-85a9-2dad933e817d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "PCM_marbastlib-xp-plate-mx:Plate_MX_1u"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "edd7cb1f-e3d1-4567-917d-f1a5be054659")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "a0031f3e-ae3c-4001-8c99-a350ee7d69ee")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted, Kailh CPG151101S11 for Cherry MX style switches"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "f06b36e7-2afd-4418-81c5-4966de94446a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/93cc7560-8cc6-4d71-93ff-7b0b79f672a9")
		(sheetname "Stammblatt")
		(sheetfile "geebord-plate.kicad_sch")
		(attr exclude_from_pos_files allow_missing_courtyard)
		(fp_rect
			(start -9.525 -9.525)
			(end 9.525 9.525)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "Dwgs.User")
			(uuid "b1327bd0-4550-4ad9-a92f-fc5eaf5ce01d")
		)
		(fp_line
			(start -7 -6.5)
			(end -7 6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "93455d42-b059-44a4-8e46-2e17bef2a4c3")
		)
		(fp_line
			(start -6.5 7)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "18024321-8e6f-4580-8e59-d0ae6df6798e")
		)
		(fp_line
			(start 6.5 -7)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "917fdea5-f59e-4346-9f10-00d1c4ff9bb9")
		)
		(fp_line
			(start 7 6.5)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "cc2b5ff0-b03a-43da-b6ae-eb09051e1dea")
		)
		(fp_arc
			(start -7 -6.5)
			(mid -6.853553 -6.853553)
			(end -6.5 -7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "72b69b58-39c9-4144-8416-165ab27a6d48")
		)
		(fp_arc
			(start -6.497236 6.998884)
			(mid -6.850789 6.852437)
			(end -6.997236 6.498884)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "24a4a0e5-3aea-41b5-9e86-1dfc92f36a8f")
		)
		(fp_arc
			(start 6.5 -7)
			(mid 6.853553 -6.853553)
			(end 7 -6.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "29e4db62-340f-4725-b71f-f60260a1400a")
		)
		(fp_arc
			(start 7 6.5)
			(mid 6.853553 6.853553)
			(end 6.5 7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "Edge.Cuts")
			(uuid "5b1af2d5-a2a5-4d31-8f3d-d44627ce9e8f")
		)
	)
	(footprint "geebord-library:Harwin_M20-89004xx_1x04_P2.54mm_Horizontal"
		(layer "B.Cu")
		(uuid "eaec1f2b-6395-4157-9fc1-dbf8efa9665c")
		(at 138.033125 99.759 -90)
		(descr "Harwin Male Horizontal Surface Mount Single Row 2.54mm (0.1 inch) Pitch PCB Connector, M20-89004xx, 4 Pins per row (https://cdn.harwin.com/pdfs/M20-890.pdf), generated with kicad-footprint-generator")
		(tags "connector Harwin M20-890 horizontal")
		(property "Reference" "J1"
			(at -0.48 6.28 90)
			(layer "B.SilkS")
			(uuid "1f153e78-84c5-4f98-9ca7-b2e62245391d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "Conn_01x04_Pin"
			(at -0.48 -6.28 90)
			(layer "B.Fab")
			(uuid "7f58bfc9-b9f4-47b0-bb4b-f60e17142f4f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Footprint" "geebord-library:Harwin_M20-89004xx_1x04_P2.54mm_Horizontal"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "418d905d-2436-464b-afd4-ba27a39ff952")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "4e81aa15-123f-4c2c-8b60-d488edda85a3")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" "Generic connector, single row, 01x04, script generated"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "4a27999f-aafc-4971-a3cd-2ee101e67a40")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/818e7c10-5692-4757-9857-1260c9195b66")
		(sheetname "Stammblatt")
		(sheetfile "geebord-plate.kicad_sch")
		(attr smd)
		(fp_line
			(start -7.095 4.63)
			(end -7.095 3.81)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "75a2e39e-42be-436e-924c-361bb3dd9c63")
		)
		(fp_line
			(start -5.525 4.63)
			(end -7.095 4.63)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "ed9d8251-ed71-4c2c-b0e1-48d1fc0d7190")
		)
		(fp_line
			(start -7.28 5.58)
			(end -7.28 -5.58)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "79ad2325-4fcb-4381-b460-910328429d3a")
		)
		(fp_line
			(start 7.28 5.58)
			(end -7.28 5.58)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "b36dcdda-55e3-4dd8-bdbe-47cb47ca4261")
		)
		(fp_line
			(start -7.28 -5.58)
			(end 7.28 -5.58)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "4e5bbfa3-829a-4b9f-be54-e5a16c9fecb3")
		)
		(fp_line
			(start 7.28 -5.58)
			(end 7.28 5.58)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "3f800fb4-ea3b-44c8-a7d4-fb7e93716d8e")
		)
		(pad "1" smd rect
			(at 0.1125 3.75 270)
			(size 13.775 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 2 "Net-(J1-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "b5e5ed95-7b6c-4e2c-b0aa-ccfbd760b8fa")
		)
		(pad "2" smd rect
			(at 0.1125 1.25 270)
			(size 13.775 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 3 "Net-(J1-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "e79697da-e8ad-4944-bb5d-3b46262cf397")
		)
		(pad "3" smd rect
			(at 0.1125 -1.25 270)
			(size 13.775 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 4 "Net-(J1-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
			(uuid "ac4280c6-1995-4fbc-9725-2bd3a29b94c7")
		)
		(pad "4" smd rect
			(at 0.1125 -3.75 270)
			(size 13.775 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "Net-(J1-Pin_4)")
			(pinfunction "Pin_4")
			(pintype "passive")
			(uuid "d4c7e384-6d49-47a6-b749-0621ff16eb4b")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_Harwin.3dshapes/Harwin_M20-89004xx_1x04_P2.54mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_arc
		(start 256.1125 25.4375)
		(mid 258.940927 26.609073)
		(end 260.1125 29.4375)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "0bfe6624-3022-4adf-a26a-f03a46603ea9")
	)
	(gr_line
		(start 16.1125 113.4375)
		(end 16.1125 29.4375)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "5ae505a9-90aa-4a62-9de8-bc15952d49e1")
	)
	(gr_arc
		(start 20.1125 117.4375)
		(mid 17.284073 116.265927)
		(end 16.1125 113.4375)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "6429d389-3db5-4702-9535-e5725a6ee523")
	)
	(gr_line
		(start 260.1125 29.4375)
		(end 260.1125 113.4375)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "7e8cc3e5-a99c-446c-8693-e3f7a3d476b4")
	)
	(gr_arc
		(start 16.1125 29.4375)
		(mid 17.284073 26.609073)
		(end 20.1125 25.4375)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "838c2254-5bc0-40ce-8141-c8637222ae2f")
	)
	(gr_arc
		(start 260.1125 113.4375)
		(mid 258.940927 116.265927)
		(end 256.1125 117.4375)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "a7c4caa7-f798-42ae-9314-396c03092dfc")
	)
	(gr_line
		(start 256.1125 117.4375)
		(end 20.1125 117.4375)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "cb6cefc4-690d-46ec-8efa-6a2cae4d6701")
	)
	(gr_line
		(start 20.1125 25.4375)
		(end 256.1125 25.4375)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "f2c633dc-30a7-4411-8246-6ebe45722280")
	)
	(gr_text "geeboard @ orangerot.dev // through the keyboard our ghosts rule the machine_"
		(at 26.4795 72.9615 0)
		(layer "B.SilkS")
		(uuid "3e22bf7f-bef9-4717-beb0-45bebbaa0528")
		(effects
			(font
				(size 2.5 2.5)
				(thickness 0.25)
			)
			(justify right bottom mirror)
		)
	)
	(gr_text "gero beckmann in 2024"
		(at 26.3525 91.8845 0)
		(layer "B.SilkS")
		(uuid "c6ea29d2-f160-4f25-8373-f3bfe4e981c6")
		(effects
			(font
				(size 2.5 2.5)
				(thickness 0.25)
				(bold yes)
			)
			(justify right bottom mirror)
		)
	)
	(segment
		(start 130.8082 101.9828)
		(end 140.0932 92.6978)
		(width 0.2)
		(layer "F.Cu")
		(net 1)
		(uuid "3d84adc1-82c1-4f2a-abf8-f2691d342421")
	)
	(segment
		(start 140.0932 92.6978)
		(end 140.0932 90.9828)
		(width 0.2)
		(layer "F.Cu")
		(net 1)
		(uuid "d5283cd5-64ec-4a1b-9d8e-bfc270dd0137")
	)
	(segment
		(start 129.0932 101.9828)
		(end 130.8082 101.9828)
		(width 0.2)
		(layer "F.Cu")
		(net 1)
		(uuid "d806b020-2aa7-40e2-9401-eff9e84c906b")
	)
	(segment
		(start 140.0932 92.484075)
		(end 141.843125 94.234)
		(width 0.2)
		(layer "B.Cu")
		(net 1)
		(uuid "65b61a61-ed00-4c0a-bc57-b108fca1a12c")
	)
	(segment
		(start 140.0932 90.9828)
		(end 140.0932 92.484075)
		(width 0.2)
		(layer "B.Cu")
		(net 1)
		(uuid "6b987b9b-5850-4fd0-9a1d-e2b500260905")
	)
	(segment
		(start 129.0932 97.9828)
		(end 136.0932 90.9828)
		(width 0.2)
		(layer "B.Cu")
		(net 2)
		(uuid "ee58b13d-b6dd-4b6a-8d26-d305e2c56fee")
	)
	(segment
		(start 138.1125 93.0275)
		(end 138.0932 93.0082)
		(width 0.2)
		(layer "B.Cu")
		(net 3)
		(uuid "03af585e-a307-4904-8f70-d1739a1a2372")
	)
	(segment
		(start 138.0932 93.0082)
		(end 138.0932 90.9828)
		(width 0.2)
		(layer "B.Cu")
		(net 3)
		(uuid "165ce252-97b3-4db6-997e-2fc209c0fc4b")
	)
	(segment
		(start 136.783125 99.8715)
		(end 136.783125 94.356875)
		(width 0.2)
		(layer "B.Cu")
		(net 3)
		(uuid "67805d78-9ffc-4f8d-93c4-dfabf2d50d5a")
	)
	(segment
		(start 136.783125 94.356875)
		(end 138.1125 93.0275)
		(width 0.2)
		(layer "B.Cu")
		(net 3)
		(uuid "aa25925e-1867-45da-8205-57cf1d58e6d8")
	)
	(segment
		(start 126.9365 100.5205)
		(end 126.9365 104.4575)
		(width 0.2)
		(layer "B.Cu")
		(net 4)
		(uuid "21537d62-5a69-409f-8a9a-0f627ef3aee8")
	)
	(segment
		(start 139.283125 106.715875)
		(end 139.283125 99.8715)
		(width 0.2)
		(layer "B.Cu")
		(net 4)
		(uuid "6060bb04-2a4d-4976-af5e-f0b24ac68077")
	)
	(segment
		(start 138.7475 107.2515)
		(end 139.283125 106.715875)
		(width 0.2)
		(layer "B.Cu")
		(net 4)
		(uuid "8aea8383-0985-4258-909b-59d2a3b0a35e")
	)
	(segment
		(start 129.7305 107.2515)
		(end 138.7475 107.2515)
		(width 0.2)
		(layer "B.Cu")
		(net 4)
		(uuid "a583d76d-83ff-4ef0-b663-d42079f2ce75")
	)
	(segment
		(start 129.0932 99.9828)
		(end 127.4742 99.9828)
		(width 0.2)
		(layer "B.Cu")
		(net 4)
		(uuid "d50a0a27-3e0d-4b21-b368-caea3550104f")
	)
	(segment
		(start 127.4742 99.9828)
		(end 126.9365 100.5205)
		(width 0.2)
		(layer "B.Cu")
		(net 4)
		(uuid "dc95fe2d-f822-493d-8a43-b0a48dc2121d")
	)
	(segment
		(start 126.9365 104.4575)
		(end 129.7305 107.2515)
		(width 0.2)
		(layer "B.Cu")
		(net 4)
		(uuid "f8954946-6f0a-4863-8465-ca143137a404")
	)
	(group ""
		(uuid "4536b9e2-c428-45f7-a63c-deac3caef1b9")
		(members "0252980b-3911-4efa-83ff-4ee7d78cf941" "0bfe6624-3022-4adf-a26a-f03a46603ea9"
			"14c3ad8e-9934-4baa-9cf0-2d89db06f535" "5ae505a9-90aa-4a62-9de8-bc15952d49e1"
			"6429d389-3db5-4702-9535-e5725a6ee523" "7e8cc3e5-a99c-446c-8693-e3f7a3d476b4"
			"808a5fc2-24f7-49c9-b720-2a501d97acbf" "838c2254-5bc0-40ce-8141-c8637222ae2f"
			"a7c4caa7-f798-42ae-9314-396c03092dfc" "cb6cefc4-690d-46ec-8efa-6a2cae4d6701"
			"cf4f5d82-6b8e-42cc-8d30-3fdde86eed05" "f2c633dc-30a7-4411-8246-6ebe45722280"
		)
	)
)
