(footprint "Harwin_M20-89004xx_1x04_P2.54mm_Horizontal" (version 20240108) (generator "pcbnew") (generator_version "8.0")
  (layer "F.Cu")
  (descr "Harwin Male Horizontal Surface Mount Single Row 2.54mm (0.1 inch) Pitch PCB Connector, M20-89004xx, 4 Pins per row (https://cdn.harwin.com/pdfs/M20-890.pdf), generated with kicad-footprint-generator")
  (tags "connector Harwin M20-890 horizontal")
  (property "Reference" "J1" (at -0.48 -6.28 180) (layer "F.SilkS")(uuid "3e9cd76c-e427-4c07-823e-197aacd6a811")
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (property "Value" "Conn_01x04_Pin" (at -0.48 6.28 180) (layer "F.Fab")(uuid "eb011bdf-185c-45ac-90e1-07bd5499f281")
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (property "Footprint" "Connector_Harwin:Harwin_M20-89004xx_1x04_P2.54mm_Horizontal" (at 0 0 0)(unlocked yes)
 (layer "F.Fab")(hide yes)
(uuid "eae3c3ee-b09c-4548-a139-7bc362854742")
    (effects (font (size 1.27 1.27) (thickness 0.15)))
  )
  (property "Datasheet" "" (at 0 0 0)(unlocked yes)
 (layer "F.Fab")(hide yes)
(uuid "d45a8709-65eb-4403-a67d-554532d5826f")
    (effects (font (size 1.27 1.27) (thickness 0.15)))
  )
  (property "Description" "Generic connector, single row, 01x04, script generated" (at 0 0 0)(unlocked yes)
 (layer "F.Fab")(hide yes)
(uuid "d7edf402-709e-4cdb-934c-da0d2c6aec4b")
    (effects (font (size 1.27 1.27) (thickness 0.15)))
  )
  (attr smd)
  (fp_line (start -7.095 -4.63) (end -5.525 -4.63)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS")(uuid "0b3b6e37-2126-41b3-a245-3fe4a9c61668"))
  (fp_line (start -7.095 -3.81) (end -7.095 -4.63)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS")(uuid "44377e0b-e0e1-4e7a-8e42-40705e2e9e6f"))
  (fp_line (start -7.28 -5.58) (end 7.28 -5.58)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd")(uuid "f1823b5c-9d25-4b96-be16-257a0866f2c7"))
  (fp_line (start -7.28 5.58) (end -7.28 -5.58)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd")(uuid "a178a175-dc10-4d24-8a18-1e73f7f02865"))
  (fp_line (start 7.28 -5.58) (end 7.28 5.58)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd")(uuid "34004b6d-c1cf-4e2f-a91e-90c6a034328c"))
  (fp_line (start 7.28 5.58) (end -7.28 5.58)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd")(uuid "1a3fe246-15d5-4a21-a9de-019cae7c4d34"))
  (pad "1" smd rect (at 0.1125 -3.75) (size 13.775 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
(uuid "2af4cd2a-6f07-4330-bc4c-25b84cfc8193")
  )
  (pad "2" smd rect (at 0.1125 -1.25) (size 13.775 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
(uuid "990532a5-00fe-44d0-b1e2-bc25ce77b890")
  )
  (pad "3" smd rect (at 0.1125 1.25) (size 13.775 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
(uuid "5ca6c5d0-cfea-4a5b-a10a-7e5836473b96")
  )
  (pad "4" smd rect (at 0.1125 3.75) (size 13.775 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
(uuid "fa5b2424-176c-4b4d-a9a0-674c5b697586")
  )
  (model "${KICAD8_3DMODEL_DIR}/Connector_Harwin.3dshapes/Harwin_M20-89004xx_1x04_P2.54mm_Horizontal.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
